{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":13,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAHG-H / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FCAHG100HVEB / RZQG100L8Y1B","FCAHG125HVEB / RZQG125L8Y1B","FCAHG140HVEB / RZQG100L8Y1B","FCAHG140HVEB / RZQG125L8Y1B","FCAHG71HVEB / FCAHG71HVEB / RZQG100L8Y1B","FCAHG71HVEB / FCAHG71HVEB / RZQG125L8Y1B","FCAHG100HVEB / RZQG71L8Y1B","FCAHG71HVEB / RZQG71L8Y1B","FCAHG140HVEB / RZQG140L7Y1B"]
["Energiatõhususe klass","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Jahutusvõimsus","Nom","","kW","","","","","","","6.80","6.80","13.40"]
["Ruumide jahutus","SEER","","","","","","","","","6.91","6.91","6.75"]
["","Aastane energiatarbimine","","kWh/a","","","","","","","345","345","1,191"]
["","Võimsus","Pdesign","kW","","","","","","","6.80","6.80","13.40"]
["","Energiatõhususe klass","","","","","","","","","A++","A++"]
["Ruumide küte (keskmine kliima)","Võimsus","Pdesign","kW","","","","","","","7.60","7.60","11.78"]
["","SCOP/A","","","","","","","","","4.54","4.54","4.38"]
["","Energiatõhususe klass","","","","","","","","","A+","A+"]
["","Aastane energiatarbimine","","kWh/a","","","","","","","2,344","2,344","3,766"]
["Nominaalne kasutegur","Energiatõhususe suhtarv","","","","","","","","","4.09","4.09","3.18"]
["Märkused","","","","","","","","","","(1) - Vt töövahemiku kohta eraldi joonist","(1) - Jahutuse nimivõimsused põhinevad: sisetemp.: 27 °CDB, 19 °CWB, välistemp.: 35 °CDB, samaväärne külmaaine torustik: 5m, kõrguste vahe: 0 m","(1) - Jahutuse nimivõimsused põhinevad: sisetemp.: 27 °CDB, 19 °CWB, välistemp.: 35 °CDB, samaväärne külmaaine torustik: 5m, kõrguste vahe: 0 m"]
["","","","","","","","","","","(2) - Vt eraldi elektriandmete joonist","(2) - Tavaliste küttevõimsuste kehtivuse tingimused: sisetemperatuur: 20 °CDB, välistemperatuur: 7 °CDB, 6 °CWB, ekvivalentne jahutustorustik: 5 m, kõrguste vahe: 0 m.","(2) - Tavaliste küttevõimsuste kehtivuse tingimused: sisetemperatuur: 20 °CDB, välistemperatuur: 7 °CDB, 6 °CWB, ekvivalentne jahutustorustik: 5 m, kõrguste vahe: 0 m."]
["Nominaalne kasutegur","Aastane energiatarve","","kWh","","","","","","","","831"]
["","COP","","","","","","","","","","4.80","4.12"]
["","Energiamärgistamise direktiiv","Jahutus","","","","","","","","","A"]
["","","Küte","","","","","","","","","A"]
["Küttevõimsus","Nom","","kW","","","","","","","","7.50","15.50"]
["Märkused","","","","","","","","","","","(3) - Vt töövahemiku kohta eraldi joonist","(3) - Vt töövahemiku kohta eraldi joonist"]
["","","","","","","","","","","","(4) - Vt eraldi elektriandmete joonist","(4) - Vt eraldi elektriandmete joonist"]
["Ruumide jahutus","ηs,c","","%","","","","","","","","","266.88"]
["Ruumide küte (keskmine kliima)","ηs,h","","%","","","","","","","","","172.10"]