{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":5,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCQ-C8 / RXS-F"]
[]
[]
[]
[]
["","","","","FCQ60C8VEB / RXS60F3V1B"]
["Jahutusvõimsus","Min","","kW","0.9"]
["","Max","","kW","6.0"]
["","Nom","","kW","5.7 (1)"]
["Torustikuühendused","Vedelik","Välisdiameeter","mm","6.35"]
["","Gaas","Välisdiameeter","mm","12.7"]
["","Tühjendus","OD","mm","32"]
["Nominaalne kasutegur","Annual energy consumption","","kWh","820"]
["","Energiatõhususe suhtarv","","","3.48"]
["","COP","","","3.52"]
["","Energiamärgistamise direktiiv","Jahutus","","A"]
["","","Küte","","B"]
["Küttevõimsus","Nom","","kW","7.0 (2)"]
["","Min","","kW","0.9"]
["","Max","","kW","8.0"]
["Märkused","","","","(1) - Jahutus: sisetemp. 27 °CDB, 19,0 °CWB; välistemp. 35 °CDB; ekvivalentne torustiku pikkus: 5 m"]
["","","","","(2) - Küte: sisetemp. 20 °CDB; välistemp. 7 °CDB, 6 °CWB; ekvivalentne jahutustorustik: 5 m"]
["","","","","(3) - Nimikasutegur: jahutus 35°/27° nominaalkoormusel, küte 7°/20° nominaalkoormusel"]