{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":7,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCQHG-F / RZQSG-L(3/8)V1"]
[]
[]
[]
[]
["","","","","FCQHG100FVEB / RZQSG100L8V1B","FCQHG125FVEB / RZQSG125L8V1B","FCQHG140FVEB / RZQSG140L7V1B"]
["Jahutusvõimsus","Nom","","kW","9.5","12.0","13.4"]
["Ruumide jahutus","SEER","","","6.70","5.40"]
["","Aastane energiatarbimine","","kWh/a","496.269","777.778"]
["","Võimsus","Pdesign","kW","9.50","12.00"]
["","Energiatõhususe klass","","","A++","A"]
["Ruumide küte (keskmine kliima)","Võimsus","Pdesign","kW","8.03","8.03"]
["","SCOP/A","","","4.30","4.10"]
["","Energiatõhususe klass","","","A+","A+"]
["","Aastane energiatarbimine","","kWh/a","2,614.419","2,741"]
["Nominaalne kasutegur","Aastane energiatarve","","kWh","1,285","1,855","2,085"]
["","Energiatõhususe suhtarv","","","3.70","3.23","3.21"]
["","COP","","","4.30","3.75","3.61"]
["","Energiamärgistamise direktiiv","Jahutus","","A","A"]
["","","Küte","","A","A"]
["Küttevõimsus","Nom","","kW","10.8","13.5","15.5"]
["Märkused","","","","(1) - EER/COP vastavalt Eurovent 2012-le, kasutamiseks ainult väljaspool EL-i","(1) - EER/COP vastavalt Eurovent 2012-le, kasutamiseks ainult väljaspool EL-i","(1) - EER/COP vastavalt Eurovent 2012-le, kasutamiseks ainult väljaspool EL-i"]
["","","","","(2) - Nimikasutegur: jahutus 35°/27° nominaalkoormusel, küte 7°/20° nominaalkoormusel","(2) - Nimikasutegur: jahutus 35°/27° nominaalkoormusel, küte 7°/20° nominaalkoormusel","(2) - Nimikasutegur: jahutus 35°/27° nominaalkoormusel, küte 7°/20° nominaalkoormusel"]