{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":116,"n_cols":9,"rows_kept":116,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCQHG-F"]
[]
[]
[]
[]
["","","","","","FCQHG71FVEB","FCQHG100FVEB","FCQHG125FVEB","FCQHG140FVEB"]
["Mürarõhutase","Küte","","kiire","dBA","","44","45","45"]
["","","","Nom","dBA","","39","40","41"]
["","","","aeglane","dBA","","33","35","37"]
["","Jahutus","","aeglane","dBA","","33","35","37"]
["","","","kiire","dBA","","44","45","45"]
["","","","Nom","dBA","","39","40","41"]
["Standardsed lisatarvikud","Kasutusjuhend","","","","","Kasutusjuhend","Kasutusjuhend","Kasutusjuhend"]
["","Paigaldusjuhend","","","","","Paigaldusjuhend","Paigaldusjuhend","Paigaldusjuhend"]
["","Tühjendusvoolik","","","","","Tühjendusvoolik","Tühjendusvoolik","Tühjendusvoolik"]
["","Tühjendusvooliku klamber","","","","","Tühjendusvooliku klamber","Tühjendusvooliku klamber","Tühjendusvooliku klamber"]
["","riputuskanduri seib","","","","","riputuskanduri seib","riputuskanduri seib","riputuskanduri seib"]
["","Kruvid","","","","","Kruvid","Kruvid","Kruvid"]
["","Liitmike isolatsioon","","","","","2","2","2"]
["","Tihenduspadjad","","","","","4","4","4"]
["","Tühjenduse tihenduspadi","","","","","Tühjenduse tihenduspadi","Tühjenduse tihenduspadi","Tühjenduse tihenduspadi"]
["","Klambrid","","","","","Klambrid","Klambrid","Klambrid"]
["Juhtsüsteemid","Juhtmega kaugjuhtimine","","","","","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B"]
["","Infrared remote control","","","","","BRC7FA532F","BRC7FA532F","BRC7FA532F"]
["Toruühendused","Vedelik","","Välisdiameeter","mm","","9.52","9.52","9.52"]
["","Gaas","","Välisdiameeter","mm","","15.9","15.9","15.9"]
["","Tühjendus","","","","","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)"]
["Ehispaneel 4","Mõõtmed","","Sügavus","mm","","50","50","50"]
["","","","Laius","mm","","950","950","950"]
["","","","Kõrgus","mm","","950","950","950"]
["","Mudel","","","","","BYCQ140D7W1 - valge, hallide restidega","BYCQ140D7W1 - valge, hallide restidega","BYCQ140D7W1 - valge, hallide restidega"]
["","Värvus","","","","","Puhas valge (RAL 9010)","Puhas valge (RAL 9010)","Puhas valge (RAL 9010)"]
["","Kaal","","","kg","","5.4","5.4","5.4"]
["Sound power level","Jahutamine","","","dBA","","61","61","61"]
["","Soojendamine","","","dBA","","61","61","61"]
["Mõõtmed","Ühik","","Laius","mm","","840","840","840"]
["","","","Sügavus","mm","","840","840","840"]
["","","","Kõrgus","mm","","288","288","288"]
["Korpus","Materjal","","","","","Galvaanitud teraplaat","Galvaanitud teraplaat","Galvaanitud teraplaat"]
["Kaal","Ühik","","","kg","","26","26","26"]
["Ehispaneel","Kaal","","","kg","","10.3","10.3","10.3"]
["","Mudel","","","","","BYCQ140D7GFW1 - isepuhastuv paneel peenesilmalisest võrgust filtriga","BYCQ140D7GFW1 - isepuhastuv paneel peenesilmalisest võrgust filtriga","BYCQ140D7GFW1 - isepuhastuv paneel peenesilmalisest võrgust filtriga"]
["","Mõõtmed","","Kõrgus","mm","","130","130","130"]
["","","","Sügavus","mm","","950","950","950"]
["","","","Laius","mm","","950","950","950"]
["","Värvus","","","","","Puhas valge (RAL 9010)","Puhas valge (RAL 9010)","Puhas valge (RAL 9010)"]
["Power supply","Faas","","","","","1~","1~","1~"]
["","Sagedus","","","Hz","","50","50","50"]
["","Nimetus","","","","","VE","VE","VE"]
["","Pinge","","","V","","220-240","220-240","220-240"]
["Märkused","","","","","","(1) - Müravõimsus on vastab müraallika poolt tekitatud müra \"võimsuse\" absoluutväärtusele.","(1) - Müravõimsus on vastab müraallika poolt tekitatud müra \"võimsuse\" absoluutväärtusele.","(1) - Müravõimsus on vastab müraallika poolt tekitatud müra \"võimsuse\" absoluutväärtusele."]
["","","","","","","(2) - BYCQ140D7W1W on valge isolatsiooniga. Valgel isolatsioonil on mustus kergemini märgatav, mille tõttu ei soovitata BYCQ140D7W1W ilupaneeli paigaldada suure mustusastmega keskkonda.","(2) - BYCQ140D7W1W on valge isolatsiooniga. Valgel isolatsioonil on mustus kergemini märgatav, mille tõttu ei soovitata BYCQ140D7W1W ilupaneeli paigaldada suure mustusastmega keskkonda.","(2) - BYCQ140D7W1W on valge isolatsiooniga. Valgel isolatsioonil on mustus kergemini märgatav, mille tõttu ei soovitata BYCQ140D7W1W ilupaneeli paigaldada suure mustusastmega keskkonda."]
["","","","","","","(3) - BYCQ140D7W1: ühtlaselt valge standardne paneel hallide restidega; BYCQ140D7W1W: ühtlaselt valge standardne paneel valgete restidega; BYCQ140D7GW1: ühtlaselt valge isepuhastuv paneel.","(3) - BYCQ140D7W1: ühtlaselt valge standardne paneel hallide restidega; BYCQ140D7W1W: ühtlaselt valge standardne paneel valgete restidega; BYCQ140D7GW1: ühtlaselt valge isepuhastuv paneel.","(3) - BYCQ140D7W1: ühtlaselt valge standardne paneel hallide restidega; BYCQ140D7W1W: ühtlaselt valge standardne paneel valgete restidega; BYCQ140D7GW1: ühtlaselt valge isepuhastuv paneel."]
["Korpus","Materjal","","","","Galvaanitud teraplaat"]
["Mõõtmed","Ühik","","Kõrgus","mm","288"]
["","","","Laius","mm","840"]
["","","","Sügavus","mm","840"]
["Kaal","Ühik","","","kg","25"]
["Ventilaator","Õhu vooluhulk","Jahutus","kiire","m³/min","21.2"]
["","","","Nom","m³/min","16.7"]
["","","","aeglane","m³/min","12.2"]
["","","Küte","kiire","m³/min","21.2"]
["","","","Nom","m³/min","16.7"]
["","","","aeglane","m³/min","12.2"]
["Helivõimsustase","Jahutamine","","","dBA","53"]
["","Soojendamine","","","dBA","53"]
["Mürarõhutase","Jahutus","","kiire","dBA","36"]
["","","","Nom","dBA","33"]
["","","","aeglane","dBA","29"]
["","Küte","","kiire","dBA","36"]
["","","","Nom","dBA","33"]
["","","","aeglane","dBA","29"]
["Toruühendused","Vedelik","","Välisdiameeter","mm","9.52"]
["","Gaas","","Välisdiameeter","mm","15.9"]
["","Tühjendus","","","","VP25 (I.D. 25/O.D. 32)"]
["Ehispaneel","Mudel","","","","BYCQ140D7GFW1 - isepuhastuv paneel peenesilmalisest võrgust filtriga"]
["","Värvus","","","","Puhas valge (RAL 9010)"]
["","Mõõtmed","","Kõrgus","mm","130"]
["","","","Laius","mm","950"]
["","","","Sügavus","mm","950"]
["","Kaal","","","kg","10.3"]
["Ehispaneel 2","Ehispaneel 2-=-Mudel","","","","BYCQ140D7GW1 - automaatselt puhastuv paneel"]
["","Värvus","","","","Puhas valge (RAL 9010)"]
["","Mõõtmed","","Kõrgus","mm","130"]
["","","","Laius","mm","950"]
["","","","Sügavus","mm","950"]
["","Kaal","","","kg","10.3"]
["Ehispaneel 3","Mudel","","","","BYCQ140D7W1W - Üleni valge"]
["","Värvus","","","","Puhas valge (RAL 9010)"]
["","Mõõtmed","","Kõrgus","mm","50"]
["","","","Laius","mm","950"]
["","","","Sügavus","mm","950"]
["","Kaal","","","kg","5.4"]
["Ehispaneel 4","Mudel","","","","BYCQ140D7W1 - valge, hallide restidega"]
["","Värvus","","","","Puhas valge (RAL 9010)"]
["","Mõõtmed","","Kõrgus","mm","950"]
["","","","Laius","mm","950"]
["","","","Sügavus","mm","50"]
["","Kaal","","","kg","5.4"]
["Juhtsüsteemid","Infrared remote control","","","","BRC7FA532F"]
["Juhtsüsteemid","Juhtmega kaugjuhtimine","","","","BRC1D52, BRC1E52A/B"]
["Standardsed lisatarvikud","Installation manual","","","","Installation manual"]
["","Washer for hanger bracket","","","","Washer for hanger bracket"]
["","Operation manual","","","","Operation manual"]
["","Clamp for drain hose","","","","Clamp for drain hose"]
["","Clamps","","","","Clamps"]
["","Drain hose","","","","Drain hose"]
["","Drain sealing pad","","","","Drain sealing pad"]
["","Installation guide","","","","Installation guide"]
["","Insulation for fitting","","","","2"]
["","Screws","","","","Screws"]
["","Sealing pads","","","","4"]
["Elektritoide","Nimetus","","","","VE"]
["","Faas","","","","1~"]
["","Elektritoide-=-Sagedus","","Sagedus","","50"]
["","Elektritoide-=-Pinge","","Pinge","","220-240"]