{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":67,"n_cols":8,"rows_kept":67,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDA-A"]
[]
[]
[]
[]
["","","","","","FDA125A5VEB","FDA200AXVEB","FDA250AXVEB"]
["Jahutusvõimsus","Üldvõimsus","","Nom","kW","12.10","19.00","22.00"]
["Küttevõimsus","Üldvõimsus","","Nom.","kW","13.50","22.4","24.0"]
["Korpus","Colour","","","","Värvimata","Värvimata","Värvimata"]
["","Materjal","","","","Galvaanitud teras","Galvaanitud teraplaat","Galvaanitud teraplaat"]
["Mõõtmed","Ühik","","Kõrgus","mm","300","470","470"]
["","","","Laius","mm","1,400","1,490","1,490"]
["","","","Sügavus","mm","700","1,100","1,100"]
["Kaal","Ühik","","","kg","45","104","115"]
["Vajalik laesüvend >","mm","","","","350"]
["Ventilaator","Õhu voolukiirus","Jahutus","kiire","m³/min","39.0","64.0","69.0"]
["","","","Keskmine","m³/min","","50","56"]
["","","","aeglane","m³/min","28.0","36.0","43.0"]
["","","Küte","kiire","m³/min","39.0","64.0","69.0"]
["","","","Keskmine","m³/min","","50.0","56.0"]
["","","","aeglane","m³/min","28.0","36.0","43.0"]
["","Väline staatiline rõhk","","Kõrge","Pa","200","250","250"]
["","","","Nom.","Pa","50","62","62"]
["Müratase","Jahutamine","","","dBA","66","69.0","71.0"]
["Helirõhu tase","Jahutus","","kiire","dBA","40","43.0","44.0"]
["","","","Keskmine","dBA","","39.0","40.0"]
["","","","aeglane","dBA","33","36.0","37.0"]
["","Küte","","kiire","dBA","40","43.0","44.0"]
["","","","Keskmine","dBA","","39.0","40.0"]
["","","","aeglane","dBA","33","36.0","37.0"]
["Toruühendused","Vedelik","","Välisdiameeter","mm","9.52","9.52","9.52"]
["","Gaas","","Välisdiameeter","mm","15.90","19.1","22.2"]
["","Tühjendus","","","","VP25 (I.D. 25/O.D. 32)","BSP1","BSP1"]
["Tühjenduskõrgus","mm","","","","625"]
["Ehispaneel","Mudel","","","","BYBS125DJW1"]
["","Värvus","","","","Valge (10Y9/0,5)"]
["","Mõõtmed","","Kõrgus","mm","55"]
["","","","Laius","mm","1,500"]
["","","","Sügavus","mm","500"]
["","Kaal","","","kg","6.5"]
["Control systems","Infrared remote control","","","","BRC4C65, BRC4C66"]
["","Wired remote control","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Standardsed lisatarvikud","Kasutusjuhend","","","","","1","1"]
["","Paigaldus- ja käitamisjuhend","","","","1","1","1"]
["","Paigaldusjuhend","","","","","1","1"]
["","Üldised ohutusmeetmed","","","","1","1","1"]
["","Gaasiühendustoru","","","","","1","1"]
["","Juhtmeklambri materjal","","","","","1","1"]
["","Seib","","","","8","12","12"]
["","Vedruseib","","","","","2","2"]
["","Kruvi + seib","","","","","45","45"]
["","Seibiga kuuskantpeaga kruvi","","","","","49","49"]
["","Kruvid","","","","16","2","2"]
["","Kuuskantpeaga kruvi","","","","","2","2"]
["","Lameseib","","","","","8","8"]
["Power supply","Nimetus","","","","","VE","VE"]
["","Phase","","","","1~","1~","1~"]
["","Sagedus","","","Hz","50/60","50/60","50/60"]
["","Pinge","","","V","220-240/220","220-240/220","220-240/220"]
["Standardsed lisatarvikud","Voolikuriba","","","","1"]
["","Tühjendusvoolik","","","","1"]
["","Juhe ühise toiteallika jaoks","","","","2"]
["","Tihendusmaterjal (äravooluvoolik)","","","","1"]
["","Tihendusmaterjal","","","","2"]
["","Soojusisolatsioonitoru (vedelik)","","","","1"]
["","Soojusisolatsioonitoru (gaas)","","","","1"]
["Märkused","","","","","(1) - Vt eraldi elektriandmete joonist"]