{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":7,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDBQ-B"]
[]
[]
[]
[]
["","","","","","FDBQ25B5V1","FDBQ25B8V1"]
["Helirõhu tase","Küte","","kiire","dBA","35.0","35.0"]
["","","","aeglane","dBA","29.0","29.0"]
["","Jahutus","","aeglane","dBA","28.0","28.0"]
["","","","kiire","dBA","35.0","35.0"]
["Standardsed lisatarvikud","Paigaldus- ja käitamisjuhend","","","","1","1"]
["","Imiõhu filter","","","","1","1"]
["Control systems","Wired remote control","","","","BRC1D52, BRC1E52A/B"]
["Piping connections","Vedelik","","Välisdiameeter","mm","6.35"]
["","Gaas","","Välisdiameeter","mm","9.52"]
["","Drain","","","","27.2"]
["Müratase","Jahutamine","","","dBA","55","55"]
["","Soojendamine","","","dBA","55","55"]
["Mõõtmed","Ühik","","Laius","mm","652","652"]
["","","","Sügavus","mm","502","502"]
["","","","Kõrgus","mm","230","230"]
["Korpus","Materjal","","","","Tsingitud madalsüsinikteras","Tsingitud madalsüsinikteras"]
["Kaal","Ühik","","","kg","17.0","17.0"]
["Ventilaator","Õhu voolukiirus","Küte","kiire","m³/min","","6.95"]
["","","","aeglane","m³/min","","5.20"]
["","","Jahutus","aeglane","m³/min","","5.20"]
["","","","kiire","m³/min","","6.50"]
["Power supply","Phase","","","","1~","1~"]
["","Sagedus","","","Hz","50","50"]
["","Nimetus","","","","V1","V1"]
["","Pinge","","","V","230","230 +/-10%"]
["Märkused","","","","","(1) - Müratasemed on mõõdetud osaliselt kajavabas testkambris.","(1) - Müratasemed on mõõdetud osaliselt kajavabas testkambris."]
["","","","","","(2) - Tegemist on mürataseme suhtelise väärtusega, mis oleneb mikrofoni kaugusest ja akustilisest keskkonnast. Lisainfot vaadake mürataseme joonistelt.","(2) - Tegemist on mürataseme suhtelise väärtusega, mis oleneb mikrofoni kaugusest ja akustilisest keskkonnast. Lisainfot vaadake mürataseme joonistelt."]
["","","","","","(3) - Müravõimsus on vastab müraallika poolt tekitatud müra \"võimsuse\" absoluutväärtusele.","(3) - Müravõimsus on vastab müraallika poolt tekitatud müra \"võimsuse\" absoluutväärtusele."]
["Piping connections","Vedelik","","Välisdiameeter","mm","","6.35"]
["","Gaas","","Välisdiameeter","mm","","9.52"]
["","Drain","","","","","27.2"]