{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":5,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDQ-B / RQ-BW1"]
[]
[]
[]
[]
["","","","","FDQ125B8V3B9 / RQ125B8W1B"]
["Jahutusvõimsus","Nom","","kW","12.5 (6)"]
["Toruühendused","Vedelik","Välisdiameeter","mm","9.52"]
["","Gaas","Välisdiameeter","mm","15.9"]
["","Drain","OD","mm","26"]
["Nominaalne kasutegur","Energiatõhususe suhtarv","","","2.61"]
["","Aastane energiatarve","","kWh","2,395"]
["","COP","","","3.24"]
["","Energiamärgistamise direktiiv","Jahutus","","D"]
["","","Küte","","C"]
["Küttevõimsus","Nom","","kW","14.6 (7)"]
["Märkused","","","","(1) - Tegemist on mürataseme suhtelise väärtusega, mis oleneb mikrofoni kaugusest ja akustilisest keskkonnast. Lisainfot vaadake mürataseme joonistelt."]
["","","","","(2) - Müravõimsus on vastab müraallika poolt tekitatud müra \"võimsuse\" absoluutväärtusele."]
["","","","","(3) - Müratasemed on mõõdetud osaliselt kajavabas testkambris."]
["","","","","(4) - Küttevõimsus kehtib ainult soojuspumbaga välisseadme korral"]
["","","","","(5) - Välisseadme tühjendustoru jaoks on vajalik torustiku tühjenduskomplekt (lisavarustus)."]
["","","","","(6) - Jahutus: sisetemp. 27 °CDB, 19 °CWB; välistemp. 35 °CDB; ekvivalentne torustiku pikkus: 7,5 m; kõrguste vahe: 0 m"]
["","","","","(7) - Küte: sisetemp. 20 °CDB; välistemp. 7 °CDB, 6 °CWB; ekvivalentne jahutustorustik: 7,5 m; kõrguste vahe: 0 m"]
["","","","","(8) - Nimikasutegur: jahutus 35°/27° nominaalkoormusel, küte 7°/20° nominaalkoormusel"]