{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":5,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDQ-B / RZQ-B9W1"]
[]
[]
[]
[]
["","","","","FDQ125B8V3B9 / RZQ125B9W1B"]
["Jahutusvõimsus","Nom","","kW","12.50 (3)"]
["Toruühendused","Vedelik","Välisdiameeter","mm","9.52"]
["","Gaas","Välisdiameeter","mm","15.9"]
["","Tühjendus","OD","mm","26"]
["Ruumide jahutus","SEER","","","3.39"]
["Nominaalne kasutegur","Aastane energiatarve","","kWh","2,075"]
["","Energiatõhususe suhtarv","","","3.01"]
["","COP","","","3.79"]
["","Energiamärgistamise direktiiv","Jahutus","","B"]
["","","Küte","","A"]
["Küttevõimsus","Nom","","kW","14.00 (4)"]
["Märkused","","","","(1) - Energiamärgis: skaala vahemikus A (kõige efektiivsem) kuni G (vähem efektiivne)"]
["","","","","(2) - Aastane energiakulu: põhineb keskmisel aastasel kasutamisel 500 töötundi täiskoormusel (nimitingimustes)"]
["","","","","(3) - Jahutus: sisetemp. 27 °CDB, 19 °CWB; välistemp. 35 °CDB; ekvivalentne torustiku pikkus: 7,5 m; kõrguste vahe: 0 m"]
["","","","","(4) - Küte: sisetemp. 20 °CDB; välistemp. 7 °CDB, 6 °CWB; ekvivalentne jahutustorustik: 7,5 m; kõrguste vahe: 0 m"]
["","","","","(5) - Nimikasutegur: jahutus 35°/27° nominaalkoormusel, küte 7°/20° nominaalkoormusel"]