{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":7,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDQ-C / RZQSG-LV1/LY1"]
[]
[]
[]
[]
["","","","","FDQ125C7VEB / RZQSG125L7V1B","FDQ125C7VEB / RZQSG125L7Y1B9","FDQ125C7VEB / RZQSG125L7Y1B"]
["Jahutusvõimsus","Nom","","kW","12.0","12.0","12.0 (3)"]
["Ruumide jahutus","SEER","","","4.35","4.35","4.35 (6)"]
["","Aastane energiatarbimine","","kWh/a","965.517","965.517"]
["","Võimsus","Pdesign","kW","12.00","12.00"]
["","Energiatõhususe klass","","","C","C"]
["Ruumide küte (keskmine kliima)","Võimsus","Pdesign","kW","7.60","7.60"]
["","SCOP/A","","","3.81","3.81","3.81 (6)"]
["","Energiatõhususe klass","","","A","A"]
["","Aastane energiatarbimine","","kWh/a","2,791","2,791"]
["Nominaalne kasutegur","Aastane energiatarve","","kWh","1,870","1,600","1,870"]
["","Energiatõhususe suhtarv","","","3.21","3.21","3.21"]
["","COP","","","3.51","3.51","3.51"]
["","Energiamärgistamise direktiiv","Jahutus","","A","A","A"]
["","","Küte","","B","B","B"]
["Küttevõimsus","Nom","","kW","13.5","13.5","13.5 (4)"]
["Märkused","","","","(1) - EER/COP vastavalt Eurovent 2012-le, kasutamiseks ainult väljaspool EL-i","(1) - EER/COP vastavalt Eurovent 2012-le, kasutamiseks ainult väljaspool EL-i","(1) - Aastane energiakulu: põhineb keskmisel aastasel kasutamisel 500 töötundi täiskoormusel (nimitingimustes)"]
["","","","","(2) - Nimikasutegur: jahutus 35°/27° nominaalkoormusel, küte 7°/20° nominaalkoormusel","(2) - Nimikasutegur: jahutus 35°/27° nominaalkoormusel, küte 7°/20° nominaalkoormusel","(2) - Energiamärgis: skaala vahemikus A (kõige efektiivsem) kuni G (vähem efektiivne)"]
["","","","","","","(3) - Jahutus: sisetemp. 27 °CDB, 19 °CWB; välistemp. 35 °CDB; ekvivalentne torustiku pikkus: 5 m; kõrguste vahe: 0 m"]
["","","","","","","(4) - Küte: sisetemp. 20 °CDB; välistemp. 7 °CDB, 6 °CWB; ekvivalentne jahutustorustik: 5 m; kõrguste vahe: 0 m"]
["","","","","","","(5) - Aastane elektritarbimine vastab energiamärgistuse direktiivile 2002/31/EÜ"]
["","","","","","","(6) - SEER ja SCOP vastavad standardile EN 14825"]
["","","","","","","(7) - Nimikasutegur: jahutus 35°/27° nominaalkoormusel, küte 7°/20° nominaalkoormusel"]