{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":15,"n_cols":6,"rows_kept":15,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F3 / 2MXM-M"]
[]
[]
[]
[]
["","","","","FDXM25F3V1B / FDXM25F3V1B / 2MXM40M3V1B","FDXM25F3V1B / FDXM35F3V1B / 2MXM40M3V1B"]
["Jahutusvõimsus","Nom","","kW","4.0","4.0"]
["Nominaalne kasutegur","Aastane energiatarve","","kWh","563","555"]
["","Energiatõhususe suhtarv","","","3.55","3.60"]
["","COP","","","4.13","4.17"]
["","Energiamärgistamise direktiiv","Jahutus","","A","A"]
["","","Küte","","A","A"]
["Küttevõimsus","Nom","","kW","4.20","4.20"]
["Märkused","","","","(1) - Jahutuse nimivõimsused põhinevad: sisetemp.: 27°CDB, 19°CWB, välistemp.: 35°CDB, samaväärne külmaaine torustik: 5 m, kõrguste vahe: 0 m Standardse tõhususega seeria andmed","(1) - Jahutuse nimivõimsused põhinevad: sisetemp.: 27°CDB, 19°CWB, välistemp.: 35°CDB, samaväärne külmaaine torustik: 5 m, kõrguste vahe: 0 m Standardse tõhususega seeria andmed"]
["","","","","(2) - Tavaliste küttevõimsuste kehtivuse tingimused: sisetemperatuur: 20 °CDB, välistemperatuur: 7 °CDB, 6 °CWB, ekvivalentne jahutustorustik: 5 m, kõrguste vahe: 0 m.","(2) - Tavaliste küttevõimsuste kehtivuse tingimused: sisetemperatuur: 20 °CDB, välistemperatuur: 7 °CDB, 6 °CWB, ekvivalentne jahutustorustik: 5 m, kõrguste vahe: 0 m."]