{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":51,"n_cols":6,"rows_kept":51,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F3 / RXM-N"]
[]
[]
[]
[]
["","","","","FDXM50F3V1B / RXM50N2V1B","FDXM60F3V1B / RXM60N2V1B"]
["Jahutusvõimsus","Min","","kW","","1.70"]
["","Nom","","kW","","6.00"]
["","Max","","kW","","6.50"]
["Küttevõimsus","Min","","kW","","1.70"]
["","Nom","","kW","","7.00"]
["","Max","","kW","","7.10"]
["Nominaalne kasutegur","Energiatõhususe suhtarv","","","","2.93"]
["","COP","","","","3.21"]
["","Aastane energiatarve","","kWh","","1,024"]
["","Energiamärgistamise direktiiv","Jahutus","","","C"]
["","","Küte","","","C"]
["Ruumide jahutus","Energiatõhususe klass","","","","A"]
["","Võimsus","Pdesign","kW","","6.00"]
["","SEER","","","","5.56"]
["","Aastane energiatarbimine","","kWh/a","","378"]
["Ruumide küte (keskmine kliima)","Energiatõhususe klass","","","","A"]
["","Võimsus","Pdesign","kW","","4.60"]
["","SCOP/A","","","","3.80"]
["","Aastane energiatarbimine","","kWh/a","","1,693"]
["Märkused","","","","","(1) - Vt töövahemiku kohta eraldi joonist"]
["","","","","","(2) - Vt eraldi elektriandmete joonist"]
["","","","","","(3) - Jahutuse nim. põhinevad: sisetemp.: 27 °CDB, 19 °CWB, välistemp.: 35 °CDB, samaväärne külmaaine torustik: 5m, kõrguste vahe: 0 m"]
["","","","","","(4) - Tavaliste küttevõimsuste kehtivuse tingimused: sisetemperatuur: 20 °CDB, välistemperatuur: 7 °CDB, 6 °CWB, ekvivalentne jahutustorustik: 5 m, kõrguste vahe: 0 m."]
["Outdoor unit","","","","RXM50N2V1B"]
["Jahutusvõimsus","Min","","kW","1.70"]
["","Nom","","kW","5.00"]
["","Max","","kW","5.30"]
["Küttevõimsus","Min","","kW","1.70"]
["","Nom","","kW","5.80"]
["","Max","","kW","6.00"]
["Nimikasutegur","Energiatõhususe suhtarv","","","3.06"]
["","COP","","","3.10"]
["","Aastane energiatarve","","kWh","816"]
["Nominaalne kasutegur","Energiamärgistamise direktiiv","Jahutus","","B"]
["","","Küte","","D"]
["Ruumide jahutus","Energiatõhususe klass","","","A+"]
["","Võimsus","Pdesign","kW","5.00"]
["","SEER","","","5.77"]
["","Aastane energiatarbimine","","kWh/a","303"]
["Ruumide küte (keskmine kliima)","Energiatõhususe klass","","","A"]
["","Võimsus","Pdesign","kW","4.00"]
["","SCOP/A","","","3.93"]
["","Pdh küttevõimsus temperatuuril -10°","","kW","3.55"]
["","Aastane energiatarbimine","","kWh/a","1424"]
["Energiatõhususe klass","","","","A+++ ~ D"]