{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":6,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F9 / RXM-R9"]
[]
[]
[]
[]
["","","","","FDXM25F3V1B9 / RXM25R5V1B9","FDXM35F3V1B9 / RXM35R5V1B9"]
["Jahutusvõimsus","Min","","kW","1.30","1.40"]
["","Nom","","kW","2.40","3.40"]
["","Max","","kW","3.00","3.80"]
["Küttevõimsus","Min","","kW","1.30","1.40"]
["","Nom","","kW","3.20","4.00"]
["","Max","","kW","4.50","5.00"]
["Nominaalne kasutegur","Energiatõhususe suhtarv","","","3.77","2.98"]
["","COP","","","4.00","3.48"]
["","Aastane energiatarve","","kWh","318","570"]
["","Energiamärgistamise direktiiv","Jahutus","","A","C"]
["","","Küte","","A","B"]
["Ruumide jahutus","Energiatõhususe klass","","","","A"]
["","Võimsus","Pdesign","kW","","3.40"]
["","SEER","","","","5.26"]
["","Aastane energiatarbimine","","kWh/a","","226"]
["Ruumide küte (keskmine kliima)","Energiatõhususe klass","","","","A"]
["","Võimsus","Pdesign","kW","","2.90"]
["","SCOP/A","","","","3.88"]
["","Aastane energiatarbimine","","kWh/a","","1,046"]
["Märkused","","","","(1) - Vt eraldi elektriandmete joonist","(1) - Jahutuse nimivõimsused põhinevad: sisetemp.: 27 °CDB, 19 °CWB, välistemp.: 35 °CDB, samaväärne külmaaine torustik: 5m, kõrguste vahe: 0 m"]
["","","","","(2) - Vt töövahemiku kohta eraldi joonist","(2) - Tavaliste küttevõimsuste kehtivuse tingimused: sisetemperatuur: 20 °CDB, välistemperatuur: 7 °CDB, 6 °CWB, ekvivalentne jahutustorustik: 5 m, kõrguste vahe: 0 m."]
["","","","","(3) - Jahutuse nimivõimsused põhinevad: sisetemp.: 27 °CDB, 19 °CWB, välistemp.: 35 °CDB, samaväärne külmaaine torustik: 5m, kõrguste vahe: 0 m","(3) - Vt töövahemiku kohta eraldi joonist"]
["","","","","(4) - Tavaliste küttevõimsuste kehtivuse tingimused: sisetemperatuur: 20 °CDB, välistemperatuur: 7 °CDB, 6 °CWB, ekvivalentne jahutustorustik: 5 m, kõrguste vahe: 0 m.","(4) - Vt eraldi elektriandmete joonist"]