{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":85,"n_cols":9,"rows_kept":85,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F9"]
[]
[]
[]
[]
["","","","","","FDXM25F3V1B9","FDXM35F3V1B9","FDXM50F3V1B9","FDXM60F3V1B9"]
["Mürarõhutase","Küte","","kiire","dBA","35.0","35.0","","38.0"]
["","","","Keskmine","dBA","33.0","33.0","","35.0"]
["","","","aeglane","dBA","27.0","27.0","","30.0"]
["","Jahutus","","Keskmine","dBA","33.0","33.0","","35.0"]
["","","","aeglane","dBA","27.0","27.0","","30.0"]
["","","","kiire","dBA","35.0","35.0","","38.0"]
["Standardsed lisatarvikud","Paigaldusjuhend","","","","1","1","","1"]
["","Kasutusjuhend","","","","1","1","","1"]
["","Liitmike isolatsioon","","","","1","1","","1"]
["","Tihenduspadi","","","","1","1","","1"]
["","Klambri metall","","","","1","1","","1"]
["","Tühjendusvoolik","","","","1","1","","1"]
["","riputuskanduri seib","","","","8","8","","8"]
["","Tihendusmaterjal","","","","2","2","","2"]
["","Klambrid","","","","6","6","","6"]
["","Kinnitusplaadi seib","","","","4","4","","4"]
["","Kanali äärikute kruvid","","","","1","1","","1"]
["","Õhufilter","","","","1","1","","1"]
["Toruühendused","Vedelik","","Välisdiameeter","mm","6.35","6.35","","6.35"]
["","Gaas","","Välisdiameeter","mm","9.50","9.50","","12.70"]
["","Tühjendus","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","","VP20 (I.D. 20/O.D. 26)"]
["Sisendvõimsus","Jahutus","","Nom","kW","0.036","0.036","","0.060"]
["","Küte","","Nom","kW","0.036","0.036","","0.060"]
["Müratase","Jahutamine","","","dBA","53.0","53.0","","56.0"]
["","Soojendamine","","","dBA","53.0","53.0","","56.0"]
["Mõõtmed","Seade","","Laius","mm","750","750","","1,150"]
["","","","Sügavus","mm","620","620","","620"]
["","","","Kõrgus","mm","200","200","","200"]
["Kaal","Ühik","","","kg","21","21","","28"]
["Ventilaator","Väline staatiline rõhk","","Nom.","Pa","30","30","","40"]
["","Õhu vooluhulk","Küte","kiire","m³/min","8.7","8.7","","16.0"]
["","","","Keskmine","m³/min","8.0","8.0","","14.8"]
["","","","aeglane","m³/min","7.3","7.3","","13.5"]
["","","Jahutus","aeglane","m³/min","7.3","7.3","","13.5"]
["","","","Keskmine","m³/min","8.0","8.0","","14.8"]
["","","","kiire","m³/min","8.7","8.7","","16.0"]
["Power supply","Faas","","","","1~","1~","","1~"]
["","Sagedus","","","Hz","50","50","","50"]
["","Pinge","","","V","220-240","220-240","","220-240"]
["Märkused","","","","","(1) - Vt eraldi elektriandmete joonist","(1) - Vt eraldi elektriandmete joonist","","(1) - Vt eraldi elektriandmete joonist"]
["Sisendvõimsus","Jahutus","","Nom","kW","","","0.060"]
["","Küte","","Nom","kW","","","0.060"]
["Mõõtmed","Ühik","","Kõrgus","mm","","","200"]
["","","","Laius","mm","","","1150"]
["","","","Sügavus","mm","","","620"]
["Kaal","Ühik","","","kg","","","28"]
["Ventilaator","Õhu vooluhulk","Jahutus","kiire","m³/min","","","15.8"]
["","Õhuvoolu kiirus","Jahutus","Keskmine","m³/min","","","14.6"]
["","","","aeglane","m³/min","","","13.3"]
["","","Küte","kiire","m³/min","","","15.8"]
["","Õhuvoolu kiirus","Küte","Keskmine","m³/min","","","14.6"]
["","","Küte","aeglane","m³/min","","","13.3"]
["","Väline staatiline rõhk","","Nom.","Pa","","","40"]
["Helivõimsustase","Jahutamine","","","dBA","","","55.0"]
["","Soojendamine","","","dBA","","","55.0"]
["Mürarõhutase","Jahutus","","kiire","dBA","","","38.0"]
["Helirõhu tase","Jahutus","","Keskmine","dBA","","","35.0"]
["Mürarõhutase","Jahutus","","aeglane","dBA","","","30.0"]
["","Küte","","kiire","dBA","","","38.0"]
["Helirõhu tase","Küte","","Keskmine","dBA","","","35.0"]
["Mürarõhutase","Küte","","aeglane","dBA","","","30.0"]
["Toruühendused","Vedelik","","Välisdiameeter","mm","","","6.35"]
["","Gaas","","Välisdiameeter","mm","","","12.70"]
["","Tühjendus","","","","","","VP20 (I.D. 20/O.D. 26)"]
["Standardsed lisatarvikud","Installation manual","","","","","","1"]
["","Washer for hanger bracket","","","","","","8"]
["","Operation manual","","","","","","1"]
["","Clamp metal","","","","","","1"]
["","Clamps","","","","","","6"]
["","Drain hose","","","","","","1"]
["","Õhufilter","","","","","","1"]
["","Insulation for fitting","","","","","","1"]
["","Screws for duct flanges","","","","","","1"]
["","Sealing material","","","","","","2"]
["","Sealing pad","","","","","","1"]
["","Washer fixing plate","","","","","","4"]
["Elektritoide","Faas","","","","","","1~"]
["","Sagedus","","","Hz","","","50"]
["","Pinge","","","V","","","220-240"]