{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":5,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXS-F9"]
[]
[]
[]
[]
["","","","","FDXS50F2VEB9"]
["Helirõhu tase","Küte","kiire","dBA","38"]
["","","Keskmine","dBA","36"]
["","","aeglane","dBA","30"]
["","Jahutus","Keskmine","dBA","36"]
["","","aeglane","dBA","30"]
["","","kiire","dBA","38"]
["Standardsed lisatarvikud","Paigaldusjuhend","","","1"]
["","Kasutusjuhend","","","1"]
["","Liitmike isolatsioon","","","1"]
["","Tihenduspadi","","","1"]
["","Klambri metall","","","1"]
["","Tühjendusvoolik","","","1"]
["","riputuskanduri seib","","","8"]
["","Tihendusmaterjal","","","2"]
["","Klambrid","","","6"]
["","Kinnitusplaadi seib","","","4"]
["","Kanali äärikute kruvid","","","1"]
["","Õhufilter","","","1"]
["Toruühendused","Vedelik","Välisdiameeter","mm","6.35"]
["","Gaas","Välisdiameeter","mm","12.7"]
["","Drain","","","VP20 (I.D. 20/O.D. 26)"]
["Sisendvõimsus","Jahutus","Nom","kW","0.060"]
["","Küte","Nom","kW","0.060"]
["Müratase","Jahutamine","","dBA","55"]
["","Soojendamine","","dBA","55"]
["Mõõtmed","Ühik","Laius","mm","1,150"]
["","","Sügavus","mm","620"]
["","","Kõrgus","mm","200"]
["Kaal","Ühik","","kg","30.0"]
["Ventilaator","Väline staatiline rõhk","Nom.","Pa","40"]
["Power supply","Phase","","","1~"]
["","Sagedus","","Hz","50/60"]
["","Nimetus","","","VE"]
["","Pinge","","V","220-240"]
["Märkused","","","","(1) - Multi-süsteemi välisseadmega ühendamisel vaadake multi-süsteemi välisseadme tehnilisi andmeid."]