{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":6,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A / RXM-N"]
[]
[]
[]
[]
["","","","","FFA50A2VEB / RXM50N2V1B","FFA60A2VEB / RXM60N2V1B"]
["Jahutusvõimsus","Nom","","kW","5.00","5.70"]
["Ruumide jahutus","Aastane energiatarbimine","","kWh/a","","347"]
["","Võimsus","Pdesign","kW","","5.70"]
["Ruumide küte (keskmine kliima)","Võimsus","Pdesign","kW","","3.96"]
["","Aastane energiatarbimine","","kWh/a","","1,372"]
["Nominaalne kasutegur","Aastane energiatarve","","kWh","771","934"]
["","Energiatõhususe suhtarv","","","3.24","3.05"]
["","COP","","","3.49","3.41"]
["","Energiamärgistamise direktiiv","Jahutus","","A","B"]
["","","Küte","","B","B"]
["Küttevõimsus","Nom","","kW","5.80","7.00"]
["Märkused","","","","(1) - Vt töövahemiku kohta eraldi joonist","(1) - Vt töövahemiku kohta eraldi joonist"]
["","","","","(2) - Vt eraldi elektriandmete joonist","(2) - Vt eraldi elektriandmete joonist"]
["","","","","(3) - Jahutuse nimivõimsused põhinevad: sisetemp.: 27 °CDB, 19 °CWB, välistemp.: 35 °CDB, samaväärne külmaaine torustik: 5m, kõrguste vahe: 0 m","(3) - Jahutuse nim. põhinevad: sisetemp.: 27 °CDB, 19 °CWB, välistemp.: 35 °CDB, samaväärne külmaaine torustik: 5m, kõrguste vahe: 0 m"]
["","","","","(4) - Tavaliste küttevõimsuste kehtivuse tingimused: sisetemperatuur: 20 °CDB, välistemperatuur: 7 °CDB, 6 °CWB, ekvivalentne jahutustorustik: 5 m, kõrguste vahe: 0 m.","(4) - Tavaliste küttevõimsuste kehtivuse tingimused: sisetemperatuur: 20 °CDB, välistemperatuur: 7 °CDB, 6 °CWB, ekvivalentne jahutustorustik: 5 m, kõrguste vahe: 0 m."]
["Ruumide jahutus","Energiatõhususe klass","","","","A+"]
["","SEER","","","","5.76"]
["Ruumide küte (keskmine kliima)","Energiatõhususe klass","","","","A+"]
["","SCOP/A","","","","4.04"]