{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":43,"n_cols":10,"rows_kept":43,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A9 / RXM-N9"]
[]
[]
[]
[]
["","","","","FFA25A2VEB9 / RXM25N2V1B9","FFA25A2VEB9 / RXM25N5V1B9","FFA35A2VEB9 / RXM35N2V1B9","FFA35A2VEB9 / RXM35N5V1B9","FFA50A2VEB9 / RXM50N2V1B9","FFA60A2VEB9 / RXM60N2V1B9"]
["Jahutusvõimsus","Nom","","kW","2.50","2.50"]
["Ruumide jahutus","SEER","","","6.17","6.17"]
["","Aastane energiatarbimine","","kWh/a","142","142"]
["","Võimsus","Pdesign","kW","2.50","2.50"]
["","Energiatõhususe klass","","","A++","A++"]
["Ruumide küte (keskmine kliima)","Võimsus","Pdesign","kW","2.31","2.31"]
["","SCOP/A","","","4.24","4.24"]
["","Energiatõhususe klass","","","A+","A+"]
["","Aastane energiatarbimine","","kWh/a","762","762"]
["Nominaalne kasutegur","Aastane energiatarve","","kWh","273","273"]
["","Energiatõhususe suhtarv","","","4.57","4.57"]
["","COP","","","3.90","3.90"]
["","Energiamärgistamise direktiiv","Jahutus","","A","A"]
["","","Küte","","A","A"]
["Küttevõimsus","Nom","","kW","3.20","3.20"]
["Märkused","","","","(1) - Vt eraldi elektriandmete joonist","(1) - Vt eraldi elektriandmete joonist"]
["","","","","(2) - Vt töövahemiku kohta eraldi joonist","(2) - Vt töövahemiku kohta eraldi joonist"]
["","","","","(3) - Jahutuse nim. põhinevad: sisetemp.: 27 °CDB, 19 °CWB, välistemp.: 35 °CDB, samaväärne külmaaine torustik: 5m, kõrguste vahe: 0 m","(3) - Jahutuse nimivõimsused põhinevad: sisetemp.: 27 °CDB, 19 °CWB, välistemp.: 35 °CDB, samaväärne külmaaine torustik: 5m, kõrguste vahe: 0 m"]
["","","","","(4) - Tavaliste küttevõimsuste kehtivuse tingimused: sisetemperatuur: 20 °CDB, välistemperatuur: 7 °CDB, 6 °CWB, ekvivalentne jahutustorustik: 5 m, kõrguste vahe: 0 m.","(4) - Tavaliste küttevõimsuste kehtivuse tingimused: sisetemperatuur: 20 °CDB, välistemperatuur: 7 °CDB, 6 °CWB, ekvivalentne jahutustorustik: 5 m, kõrguste vahe: 0 m."]
["Välisseade","","","","","","RXM35N2V1B9","RXM35N5V1B9","","RXM60N2V1B9"]
["Jahutusvõimsus","Nom","","kW","","","3.40","3.40","5.00","5.70"]
["Küttevõimsus","Nom","","kW","","","4.20","4.20","5.80","7.00"]
["Nimikasutegur","Energiatõhususe suhtarv","","","","","3.81","3.81","3.24","3.05"]
["","COP","","","","","3.50","3.50","3.49","3.41"]
["","Aastane energiatarve","","kWh","","","446","446","772","934"]
["Nominaalne kasutegur","Energiamärgistamise direktiiv","Jahutus","","","","A","A","A","B"]
["","","Küte","","","","B","B","B","B"]
["Ruumide jahutus","Energiatõhususe klass","","","","","A++","A++","A+","A+"]
["","Võimsus","Pdesign","kW","","","3.40","3.40","5.00","5.70"]
["","SEER","","","","","6.38","6.38","5.98","5.76"]
["","Aastane energiatarbimine","","kWh/a","","","186","186","293","347"]
["Ruumide küte (keskmine kliima)","Energiatõhususe klass","","","","","A+","A+","A","A+"]
["","Võimsus","Pdesign","kW","","","3.10","3.10","3.84","3.96"]
["","SCOP/A","","","","","4.10","4.10","3.90","4.04"]
["","Pdh küttevõimsus temperatuuril -10°","","kW","","","2.04","2.04","3.40","3.66"]
["","Aastane energiatarbimine","","kWh/a","","","1058","1058","1378","1372"]
["Energiatõhususe klass","","","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]