{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":9,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A9 / RZAG-A"]
[]
[]
[]
[]
["","","","","FFA35A2VEB9 / RZAG35A2V1B","FFA50A2VEB9 / RZAG35A2V1B","FFA50A2VEB9 / RZAG50A2V1B","FFA60A2VEB9 / RZAG50A2V1B","FFA60A2VEB9 / RZAG60A2V1B"]
["Jahutusvõimsus","Min","","kW","1.6","1.6","1.7","1.7","1.7"]
["","Max","","kW","4.5","4.5","6.0","6.0","6.5"]
["","Nom","","kW","3.5","3.5","5.0","5.0","6.0"]
["Ruumide jahutus","SEER","","","6.40","6.81","6.30","6.43","5.80"]
["","Aastane energiatarbimine","","kWh/a","191","180","278","272","362"]
["","Võimsus","Pdesign","kW","3.50","3.50","5.00","5.00","6.00"]
["","Energiatõhususe klass","","","A++","A++","A++","A++","A+"]
["Ruumide küte (keskmine kliima)","Võimsus","Pdesign","kW","4.20","4.20","4.30","4.30","4.50"]
["","SCOP/A","","","3.80","4.04","4.01","4.08","4.04"]
["","Energiatõhususe klass","","","A","A+","A+","A+","A+"]
["","Aastane energiatarbimine","","kWh/a","1,546","1,455","1,501","1,474","1,558"]
["Nominaalne kasutegur","Aastane energiatarve","","kWh","438","412","735","691","929"]
["","Energiatõhususe suhtarv","","","4.00","4.25","3.40","3.62","3.23"]
["","COP","","","3.71","3.94","3.10","3.15","2.90"]
["","Energiamärgistamise direktiiv","Jahutus","","A","A","A","A","A"]
["","","Küte","","A","A","D","D","D"]
["Küttevõimsus","Nom","","kW","4.00","4.00","5.80","5.80","7.00"]
["","Min","","kW","1.40","1.40","1.50","1.50","1.60"]
["","Max","","kW","5.00","5.00","6.00","6.00","7.50"]