{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":14,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A9 / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FFA35A2VEB9 / FFA35A2VEB9 / FFA35A2VEB9 / RZQG100L8Y1B","FFA35A2VEB9 / FFA35A2VEB9 / FFA35A2VEB9 / FFA35A2VEB9 / RZQG125L8Y1B","FFA50A2VEB9 / FFA50A2VEB9 / FFA50A2VEB9 / RZQG125L8Y1B","FFA50A2VEB9 / FFA50A2VEB9 / RZQG100L8Y1B","FFA60A2VEB9 / FFA60A2VEB9 / RZQG125L8Y1B","FFA35A2VEB9 / FFA35A2VEB9 / FFA35A2VEB9 / FFA35A2VEB9 / RZQG100L8Y1B","FFA50A2VEB9 / FFA50A2VEB9 / FFA50A2VEB9 / RZQG100L8Y1B","FFA35A2VEB9 / FFA35A2VEB9 / FFA35A2VEB9 / RZQG71L8Y1B","FFA35A2VEB9 / FFA35A2VEB9 / RZQG71L8Y1B","FFA50A2VEB9 / FFA50A2VEB9 / RZQG71L8Y1B"]
["Energiatõhususe klass","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Jahutusvõimsus","Nom","","kW","","","","","","","","6.80","6.80","6.80"]
["Ruumide jahutus","SEER","","","","","","","","","","5.10","5.10","5.10"]
["","Aastane energiatarbimine","","kWh/a","","","","","","","","467","467","467"]
["","Võimsus","Pdesign","kW","","","","","","","","6.80","6.80","6.80"]
["","Energiatõhususe klass","","","","","","","","","","A","A","A"]
["Ruumide küte (keskmine kliima)","Võimsus","Pdesign","kW","","","","","","","","6.00","6.00","6.00"]
["","SCOP/A","","","","","","","","","","3.80","3.80","3.80"]
["","Energiatõhususe klass","","","","","","","","","","A","A","A"]
["","Aastane energiatarbimine","","kWh/a","","","","","","","","2,211","2,211","2,211"]
["Nominaalne kasutegur","Energiatõhususe suhtarv","","","","","","","","","","3.38","3.38","3.38"]
["Märkused","","","","","","","","","","","(1) - Vt töövahemiku kohta eraldi joonist","(1) - Jahutuse nimivõimsused põhinevad: sisetemp.: 27 °CDB, 19 °CWB, välistemp.: 35 °CDB, samaväärne külmaaine torustik: 5m, kõrguste vahe: 0 m","(1) - Vt töövahemiku kohta eraldi joonist"]
["","","","","","","","","","","","(2) - Vt eraldi elektriandmete joonist","(2) - Tavaliste küttevõimsuste kehtivuse tingimused: sisetemperatuur: 20 °CDB, välistemperatuur: 7 °CDB, 6 °CWB, ekvivalentne jahutustorustik: 5 m, kõrguste vahe: 0 m.","(2) - Vt eraldi elektriandmete joonist"]
["","","","","","","","","","","","","(3) - Vt töövahemiku kohta eraldi joonist"]
["","","","","","","","","","","","","(4) - Vt eraldi elektriandmete joonist"]