{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":18,"n_cols":6,"rows_kept":18,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFQ-B9V / RXS-F"]
[]
[]
[]
[]
["","","","","FFQ60B9V1B / RXS60F3V1B","FFQ60B9V1B / RXS60F4V1B"]
["Jahutusvõimsus","Nom","","kW","5.80 (3)","5.80 (3)"]
["Nominaalne kasutegur","Annual energy consumption","","kWh","1,035","1,035"]
["","Energiatõhususe suhtarv","","","2.80","2.80"]
["","COP","","","2.81","2.81"]
["","Energiamärgistamise direktiiv","Jahutus","","D","D"]
["","","Küte","","D","D"]
["Küttevõimsus","Nom","","kW","7.00 (4)","7.00 (4)"]
["Märkused","","","","(1) - Energiamärgis: skaala vahemikus A (kõige efektiivsem) kuni G (vähem efektiivne)","(1) - EER/COP vastavalt Eurovent 2012-le, kasutamiseks ainult väljaspool EL-i"]
["","","","","(2) - Aastane energiakulu: põhineb keskmisel aastasel kasutamisel 500 töötundi täiskoormusel (nimitingimustes)","(2) - Nimikasutegur: jahutus 35°/27° nominaalkoormusel, küte 7°/20° nominaalkoormusel"]
["","","","","(3) - Jahutus: sisetemp. 27 °CDB, 19 °CWB; välistemp. 35 °CDB; ekvivalentne torustiku pikkus: 7,5 m; kõrguste vahe: 0 m"]
["","","","","(4) - Küte: sisetemp. 20 °CDB; välistemp. 7 °CDB, 6 °CWB; ekvivalentne jahutustorustik: 7,5 m; kõrguste vahe: 0 m"]
["","","","","(5) - Nimikasutegur: jahutus 35°/27° nominaalkoormusel, küte 7°/20° nominaalkoormusel"]