{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":6,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A(9) / RXM-A9"]
[]
[]
[]
[]
["","","","","FHA35AVEB98 / RXM35A5V1B9","FHA50AVEB98 / RXM50A5V1B9"]
["Jahutusvõimsus","Nom","","kW","3.4","5"]
["Küttevõimsus","Nom","","kW","4","6"]
["Nimikasutegur","Energiatõhususe suhtarv","","","3.73","3.21"]
["","COP","","","4.08","3.35"]
["","Aastane energiatarve","","kWh","456","779"]
["Nominaalne kasutegur","Energiamärgistamise direktiiv","Jahutus","","A","A"]
["","","Küte","","A","C"]
["Ruumide jahutus","Energiatõhususe klass","","","A++","A+"]
["","Võimsus","Pdesign","kW","3.4","5"]
["","SEER","","","6.31","5.92"]
["","Aastane energiatarbimine","","kWh/a","189","295"]
["Ruumide küte (keskmine kliima)","Energiatõhususe klass","","","A+","A"]
["","Võimsus","Pdesign","kW","3.1","4.35"]
["","SCOP/A","","","4.48","3.86"]
["","Pdh küttevõimsus temperatuuril -10°","","kW","2.47","3.85"]
["","Aastane energiatarbimine","","kWh/a","968","1577"]
["Energiatõhususe klass","","","","A+++ ~ D","A+++ ~ D"]
["Märkused","","","","(1) - Vt töövahemiku kohta eraldi joonist","(1) - Jahutuse nim. põhinevad: sisetemp.: 27 °CDB, 19 °CWB, välistemp.: 35 °CDB, samaväärne külmaaine torustik: 5m, kõrguste vahe: 0 m"]
["","","","","(2) - Vt eraldi elektriandmete joonist","(2) - Tavaliste küttevõimsuste kehtivuse tingimused: sisetemperatuur: 20 °CDB, välistemperatuur: 7 °CDB, 6 °CWB, ekvivalentne jahutustorustik: 5 m, kõrguste vahe: 0 m."]
["","","","","(3) - Jahutuse nim. põhinevad: sisetemp.: 27 °CDB, 19 °CWB, välistemp.: 35 °CDB, samaväärne külmaaine torustik: 5m, kõrguste vahe: 0 m","(3) - Vt töövahemiku kohta eraldi joonist"]
["","","","","(4) - Tavaliste küttevõimsuste kehtivuse tingimused: sisetemperatuur: 20 °CDB, välistemperatuur: 7 °CDB, 6 °CWB, ekvivalentne jahutustorustik: 5 m, kõrguste vahe: 0 m.","(4) - Vt eraldi elektriandmete joonist"]