{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":7,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A(9) / RXM-R9"]
[]
[]
[]
[]
["","","","","FHA35AVEB99 / RXM35R5V1B9","FHA35AVEB98 / RXM35R5V1B9","FHA35AVEB9 / RXM35R5V1B9"]
["Jahutusvõimsus","Nom","","kW","3.40","3.40","3.40"]
["Küttevõimsus","Nom","","kW","4.00","4.00","4.00"]
["Nominaalne kasutegur","Aastane energiatarve","","kWh","456","456","456"]
["","COP","","","4.08","4.08","4.08"]
["","Energiatõhususe suhtarv","","","3.73","3.73","3.73"]
["","Energiamärgistamise direktiiv","Jahutus","","A","A","A"]
["","","Küte","","A","A","A"]
["Ruumide jahutus","Aastane energiatarbimine","","kWh/a","","","191"]
["","Võimsus","Pdesign","kW","","","3.40"]
["Ruumide küte (keskmine kliima)","Aastane energiatarbimine","","kWh/a","","","979"]
["","Võimsus","Pdesign","kW","","","3.10"]
["Märkused","","","","(1) - Jahutuse nimivõimsused põhinevad: sisetemp.: 27 °CDB, 19 °CWB, välistemp.: 35 °CDB, samaväärne külmaaine torustik: 5m, kõrguste vahe: 0 m","(1) - Jahutuse nimivõimsused põhinevad: sisetemp.: 27 °CDB, 19 °CWB, välistemp.: 35 °CDB, samaväärne külmaaine torustik: 5m, kõrguste vahe: 0 m","(1) - Jahutuse nimivõimsused põhinevad: sisetemp.: 27 °CDB, 19 °CWB, välistemp.: 35 °CDB, samaväärne külmaaine torustik: 5m, kõrguste vahe: 0 m"]
["","","","","(2) - Tavaliste küttevõimsuste kehtivuse tingimused: sisetemperatuur: 20 °CDB, välistemperatuur: 7 °CDB, 6 °CWB, ekvivalentne jahutustorustik: 5 m, kõrguste vahe: 0 m.","(2) - Tavaliste küttevõimsuste kehtivuse tingimused: sisetemperatuur: 20 °CDB, välistemperatuur: 7 °CDB, 6 °CWB, ekvivalentne jahutustorustik: 5 m, kõrguste vahe: 0 m.","(2) - Tavaliste küttevõimsuste kehtivuse tingimused: sisetemperatuur: 20 °CDB, välistemperatuur: 7 °CDB, 6 °CWB, ekvivalentne jahutustorustik: 5 m, kõrguste vahe: 0 m."]
["","","","","(3) - Vt töövahemiku kohta eraldi joonist","(3) - Vt töövahemiku kohta eraldi joonist","(3) - Vt töövahemiku kohta eraldi joonist"]
["","","","","(4) - Vt eraldi elektriandmete joonist","(4) - Vt eraldi elektriandmete joonist","(4) - Vt eraldi elektriandmete joonist"]
["Ruumide jahutus","Energiatõhususe klass","","","","","A++"]
["","SEER","","","","","6.24"]
["Ruumide küte (keskmine kliima)","Energiatõhususe klass","","","","","A+"]
["","SCOP/A","","","","","4.43"]