{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":7,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A / RXM-M9"]
[]
[]
[]
[]
["","","","","FHA35AVEB / RXM35M3V1B9","FHA50AVEB / RXM50M3V1B9","FHA60AVEB / RXM60M3V1B9"]
["Jahutusvõimsus","Nom","","kW","3.40"]
["Ruumide jahutus","SEER","","","6.24"]
["","Aastane energiatarbimine","","kWh/a","191"]
["","Võimsus","Pdesign","kW","3.40"]
["","Energiatõhususe klass","","","A++"]
["Ruumide küte (keskmine kliima)","Võimsus","Pdesign","kW","3.10"]
["","SCOP/A","","","4.43"]
["","Energiatõhususe klass","","","A+"]
["","Aastane energiatarbimine","","kWh/a","979"]
["Nominaalne kasutegur","Aastane energiatarve","","kWh","456"]
["","Energiatõhususe suhtarv","","","3.73"]
["","COP","","","4.08"]
["","Energiamärgistamise direktiiv","Jahutus","","A"]
["","","Küte","","A"]
["Küttevõimsus","Nom","","kW","4.00"]
["Märkused","","","","(1) - Vt eraldi elektriandmete joonist"]
["","","","","(2) - Vt töövahemiku kohta eraldi joonist"]
["","","","","(3) - Jahutuse nim. põhinevad: sisetemp.: 27 °CDB, 19 °CWB, välistemp.: 35 °CDB, samaväärne külmaaine torustik: 5m, kõrguste vahe: 0 m"]
["","","","","(4) - Tavaliste küttevõimsuste kehtivuse tingimused: sisetemperatuur: 20 °CDB, välistemperatuur: 7 °CDB, 6 °CWB, ekvivalentne jahutustorustik: 5 m, kõrguste vahe: 0 m."]
["Outdoor unit","","","","","RXM50M3V1B9","RXM60M3V1B9"]
["Jahutusvõimsus","Nom","","kW","","5.00","5.70"]
["Küttevõimsus","Nom","","kW","","6.00","7.20"]
["Nimikasutegur","Energiatõhususe suhtarv","","","","3.21","3.29"]
["","COP","","","","3.35","3.32"]
["","Aastane energiatarve","","kWh","","780","867"]
["Nominaalne kasutegur","Energiamärgistamise direktiiv","Jahutus","","","B","A"]
["","","Küte","","","C","C"]
["Ruumide jahutus","Energiatõhususe klass","","","","A+","A+"]
["","Võimsus","Pdesign","kW","","5.00","5.70"]
["","SEER","","","","5.92","6.08"]
["","Aastane energiatarbimine","","kWh/a","","295","328"]
["Ruumide küte (keskmine kliima)","Energiatõhususe klass","","","","A","A"]
["","Võimsus","Pdesign","kW","","4.35","4.71"]
["","SCOP/A","","","","3.86","3.87"]
["","Pdh küttevõimsus temperatuuril -10°","","kW","","3.85","4.08"]
["","Aastane energiatarbimine","","kWh/a","","1578","1704"]