{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":8,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A"]
[]
[]
[]
[]
["","","","","FHA35AVEB","FHA50AVEB","FHA60AVEB","FHA71AVEB"]
["Mürarõhutase","Küte","kiire","dBA","36","37","37","38"]
["","","Nom","dBA","34","35","35","36"]
["","","Keskmine","dBA","31","32","33","34"]
["","Jahutus","Keskmine","dBA","34","35","35","36"]
["","","aeglane","dBA","31","32","33","34"]
["","","kiire","dBA","36","37","37","38"]
["Standardsed lisatarvikud","Torustiku termoisolatsioon","","","2","2","2","2"]
["","Juhtmeklambri materjal","","","7","7","7","7"]
["","Voolikuriba","","","1","1","1","1"]
["","Tühjendusvoolik","","","1","1","1","1"]
["","Seib","","","8","8","8","8"]
["","Tihenduspadi (suur)","","","1","1","1","1"]
["","Tihenduspadi (väike)","","","1","1","1","1"]
["","Vaigust puks","","","1","1","1","1"]
["","Kruvid","","","2","2","2","2"]
["","Juhtmeklamber","","","2","2","2","2"]
["Juhtsüsteemid","Wired remote control","","","BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1D528, BRC1E51A7","BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1D528, BRC1E51A7","BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1D528, BRC1E51A7","BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1D528, BRC1E51A7"]
["","Infrared remote control","","","BRC7GA53, BRC7GA56","BRC7GA53, BRC7GA56","BRC7GA53, BRC7GA56","BRC7GA53, BRC7GA56"]
["Toruühendused","Vedelik","Välisdiameeter","mm","6.35","6.35","6.35","9.52"]
["","Gaas","Välisdiameeter","mm","9.50","12.7","12.7","15.9"]
["","Drain","","","VP20","VP20","VP20","VP20"]
["Müratase","Jahutamine","","dBA","53","54","54","55"]
["Mõõtmed","Seade","Laius","mm","960","960","1,270","1,270"]
["","","Sügavus","mm","690","690","690","690"]
["","","Kõrgus","mm","235","235","235","235"]
["Korpus","Materjal","","","Vaik, lehtmetall","Vaik, lehtmetall","Vaik, lehtmetall","Vaik, lehtmetall"]
["","Colour","","","Valge","Valge","Valge","Valge"]
["Kaal","Ühik","","kg","24.0","25.0","31.0","32.0"]
["Power supply","Faas","","","1~","1~","1~","1~"]
["","Sagedus","","Hz","50","50","50","50"]
["","Pinge","","V","220-240","220-240","220-240","220-240"]
["Märkused","","","","(1) - Vt eraldi elektriandmete joonist","(1) - Vt eraldi elektriandmete joonist","(1) - Vt eraldi elektriandmete joonist","(1) - Vt eraldi elektriandmete joonist"]