{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":5,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHQ-B8 / RXS-F"]
[]
[]
[]
[]
["","","","","FHQ60BWV1B / RXS60F3V1B"]
["Jahutusvõimsus","Min","","kW","1.7"]
["","Max","","kW","6.0"]
["","Nom","","kW","5.7 (3)"]
["Toruühendused","Vedelik","Välisdiameeter","mm","6.35"]
["","Gaas","Välisdiameeter","mm","12.7"]
["","Tühjendus","OD","mm","VP20 (Välisdiam. 26, sisediam. 20)"]
["Nominaalne kasutegur","Aastane energiatarve","","kWh","1,075"]
["","Energiatõhususe suhtarv","","","2.65"]
["","COP","","","2.89"]
["","Energiamärgistamise direktiiv","Jahutus","","D"]
["","","Küte","","D"]
["Küttevõimsus","Nom","","kW","7.2 (4)"]
["","Min","","kW","1.7"]
["","Max","","kW","8.0"]
["Märkused","","","","(1) - Energiamärgis: skaala vahemikus A (kõige efektiivsem) kuni G (vähem efektiivne)"]
["","","","","(2) - Aastane energiakulu: põhineb keskmisel aastasel kasutamisel 500 töötundi täiskoormusel (nimitingimustes)"]
["","","","","(3) - Jahutus: sisetemp. 27 °CDB, 19,0 °CWB; välistemp. 35 °CDB, 24 °CWB; ekvivalentne torustiku pikkus: 5 m"]
["","","","","(4) - Küte: sisetemp. 20 °CDB; välistemp. 7 °CDB, 6 °CWB; ekvivalentne jahutustorustik: 5 m"]
["","","","","(5) - Nimikasutegur: jahutus 35°/27° nominaalkoormusel, küte 7°/20° nominaalkoormusel"]