{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":11,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHQ-C"]
[]
[]
[]
[]
["","","","","FHQ35CAVEB","FHQ50CAVEB","FHQ60CAVEB","FHQ71CAVEB","FHQ100CAVEB","FHQ125CAVEB","FHQ140CAVEB"]
["Mürarõhutase","Küte","kiire","dBA","36","37","37","38","42","44","46"]
["","","Nom","dBA","34","35","35","36","38","41","42"]
["","","aeglane","dBA","31","32","33","34","34","37","38"]
["","Jahutus","aeglane","dBA","31","32","33","34","34","37","38"]
["","","kiire","dBA","36","37","37","38","42","44","46"]
["","","Nom","dBA","34","35","35","36","38","41","42"]
["Standardsed lisatarvikud","Paigaldusjuhend","","","Paigaldusjuhend","Paigaldusjuhend","Paigaldusjuhend","Paigaldusjuhend","Paigaldusjuhend","Paigaldusjuhend","Paigaldusjuhend"]
["","Kasutusjuhend","","","Kasutusjuhend","Kasutusjuhend","Kasutusjuhend","Kasutusjuhend","Kasutusjuhend","Kasutusjuhend","Kasutusjuhend"]
["","Vastavusdeklaratsioon","","","Vastavusdeklaratsioon","Vastavusdeklaratsioon","Vastavusdeklaratsioon","Vastavusdeklaratsioon","Vastavusdeklaratsioon","Vastavusdeklaratsioon","Vastavusdeklaratsioon"]
["","Tühjendusvoolik","","","Tühjendusvoolik","Tühjendusvoolik","Tühjendusvoolik","Tühjendusvoolik","Tühjendusvoolik","Tühjendusvoolik","Tühjendusvoolik"]
["","Klambri metall","","","Klambri metall","Klambri metall","Klambri metall","Klambri metall","Klambri metall","Klambri metall","Klambri metall"]
["","riputuskanduri seib","","","riputuskanduri seib","riputuskanduri seib","riputuskanduri seib","riputuskanduri seib","riputuskanduri seib","riputuskanduri seib","riputuskanduri seib"]
["","Klambrid","","","Klambrid","Klambrid","Klambrid","Klambrid","Klambrid","Klambrid","Klambrid"]
["","Paigaldusšabloon","","","Paigaldusšabloon","Paigaldusšabloon","Paigaldusšabloon","Paigaldusšabloon","Paigaldusšabloon","Paigaldusšabloon","Paigaldusšabloon"]
["","Liitmiku isolatsioonimaterjal","","","Liitmiku isolatsioonimaterjal","Liitmiku isolatsioonimaterjal","Liitmiku isolatsioonimaterjal","Liitmiku isolatsioonimaterjal","Liitmiku isolatsioonimaterjal","Liitmiku isolatsioonimaterjal","Liitmiku isolatsioonimaterjal"]
["","Tihendusmaterjal","","","Tihendusmaterjal","Tihendusmaterjal","Tihendusmaterjal","Tihendusmaterjal","Tihendusmaterjal","Tihendusmaterjal","Tihendusmaterjal"]
["","Vaigust puks","","","Vaigust puks","Vaigust puks","Vaigust puks","Vaigust puks","Vaigust puks","Vaigust puks","Vaigust puks"]
["","Juhtmeklamber","","","Juhtmeklamber","Juhtmeklamber","Juhtmeklamber","Juhtmeklamber","Juhtmeklamber","Juhtmeklamber","Juhtmeklamber"]
["","Juhtmeklambri kruvi","","","Juhtmeklambri kruvi","Juhtmeklambri kruvi","Juhtmeklambri kruvi","Juhtmeklambri kruvi","Juhtmeklambri kruvi","Juhtmeklambri kruvi","Juhtmeklambri kruvi"]
["Juhtsüsteemid","Juhtmega kaugjuhtimine","","","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B"]
["","Infrared remote control","","","BRC7G53","BRC7G53","BRC7G53","BRC7G53","BRC7G53","BRC7G53","BRC7G53"]
["Toruühendused","Vedelik","Välisdiameeter","mm","6.35","6.35","6.35","9.52","9.52","9.52","9.52"]
["","Gaas","Välisdiameeter","mm","9.5","12.7","12.7","15.9","15.9","15.9","15.9"]
["","Tühjendus","","","VP20","VP20","VP20","VP20","VP20","VP20","VP20"]
["Sound power level","Jahutamine","","dBA","53","54","54","55","60","62","64"]
["","Soojendamine","","dBA","53","54","54","55","60","62","64"]
["Mõõtmed","Ühik","Laius","mm","960","960","1,270","1,270","1,590","1,590","1,590"]
["","","Sügavus","mm","690","690","690","690","690","690","690"]
["","","Kõrgus","mm","235","235","235","235","235","235","235"]
["Korpus","Materjal","","","Vaik, lehtmetall","Vaik, lehtmetall","Vaik, lehtmetall","Vaik, lehtmetall","Vaik, lehtmetall","Vaik, lehtmetall","Vaik, lehtmetall"]
["","Värvus","","","Värske valge","Värske valge","Värske valge","Värske valge","Värske valge","Värske valge","Värske valge"]
["Kaal","Ühik","","kg","24","25","31","32","38","38","38"]
["Power supply","Faas","","","1~","1~","1~","1~","1~","1~","1~"]
["","Sagedus","","Hz","50/60","50/60","50/60","50/60","50/60","50/60","50/60"]
["","Nimetus","","","VE","VE","VE","VE","VE","VE","VE"]
["","Pinge","","V","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220"]