{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":48,"n_cols":12,"rows_kept":48,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHQ-C"]
[]
[]
[]
[]
["","","","","","FHQ35CAVEB (Archived)","FHQ50CAVEB (Archived)","FHQ60CAVEB (Archived)","FHQ71CAVEB (Archived)","FHQ100CAVEB (Archived)","FHQ125CAVEB (Archived)","FHQ140CAVEB (Archived)"]
["Korpus","Värvus","","","","Värske valge","Värske valge","Värske valge","Värske valge","Värske valge","Värske valge","Värske valge"]
["","Materjal","","","","Vaik, lehtmetall","Vaik, lehtmetall","Vaik, lehtmetall","Vaik, lehtmetall","Vaik, lehtmetall","Vaik, lehtmetall","Vaik, lehtmetall"]
["Mõõtmed","Ühik","","Kõrgus","mm","235","235","235","235","235","235","235"]
["","","","Laius","mm","960","960","1270","1270","1590","1590","1590"]
["","","","Sügavus","mm","690","690","690","690","690","690","690"]
["Kaal","Ühik","","","kg","24","25","31","32","38","38","38"]
["Ventilaator","Õhu vooluhulk","Jahutus","kiire","m³/min","14","15","19.5","20.5","28","31","34"]
["","","","Nom","m³/min","11.5","12","15","17","24","27","29"]
["","","","aeglane","m³/min","10","10","11.5","14","20","23","24"]
["","","Küte","kiire","m³/min","14","15","19.5","20.5","28","31","34"]
["","","","Nom","m³/min","11.5","12","15","17","24","27","29"]
["","","","aeglane","m³/min","10","10","11.5","14","20","23","24"]
["Helivõimsustase","Jahutamine","","","dBA","53","54","54","55","60","62","64"]
["","Soojendamine","","","dBA","53","54","54","55","60","62","64"]
["Mürarõhutase","Jahutus","","kiire","dBA","36","37","37","38","42","44","46"]
["","","","Nom","dBA","34","35","35","36","38","41","42"]
["","","","aeglane","dBA","31","32","33","34","34","37","38"]
["","Küte","","kiire","dBA","36","37","37","38","42","44","46"]
["","","","Nom","dBA","34","35","35","36","38","41","42"]
["","","","aeglane","dBA","31","32","33","34","34","37","38"]
["Toruühendused","Vedelik","","Välisdiameeter","mm","6.35","6.35","6.35","9.52","9.52","9.52","9.52"]
["","Gaas","","Välisdiameeter","mm","9.5","12.7","12.7","15.9","15.9","15.9","15.9"]
["","Tühjendus","","","","VP20","VP20","VP20","VP20","VP20","VP20","VP20"]
["Juhtsüsteemid","Infrapunakaugjuhtimine","","","","BRC7G53","BRC7G53","BRC7G53","BRC7G53","BRC7G53","BRC7G53","BRC7G53"]
["","Juhtmega kaugjuhtimine","","","","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B"]
["Standardsed lisatarvikud","Paigaldusjuhend","","","","Paigaldusjuhend","Paigaldusjuhend","Paigaldusjuhend","Paigaldusjuhend","Paigaldusjuhend","Paigaldusjuhend","Paigaldusjuhend"]
["","riputuskanduri seib","","","","riputuskanduri seib","riputuskanduri seib","riputuskanduri seib","riputuskanduri seib","riputuskanduri seib","riputuskanduri seib","riputuskanduri seib"]
["","Liitmiku isolatsioonimaterjal","","","","Liitmiku isolatsioonimaterjal","Liitmiku isolatsioonimaterjal","Liitmiku isolatsioonimaterjal","Liitmiku isolatsioonimaterjal","Liitmiku isolatsioonimaterjal","Liitmiku isolatsioonimaterjal","Liitmiku isolatsioonimaterjal"]
["","Vaigust puks","","","","Vaigust puks","Vaigust puks","Vaigust puks","Vaigust puks","Vaigust puks","Vaigust puks","Vaigust puks"]
["","Juhtmeklamber","","","","Juhtmeklamber","Juhtmeklamber","Juhtmeklamber","Juhtmeklamber","Juhtmeklamber","Juhtmeklamber","Juhtmeklamber"]
["","Juhtmeklambri kruvi","","","","Juhtmeklambri kruvi","Juhtmeklambri kruvi","Juhtmeklambri kruvi","Juhtmeklambri kruvi","Juhtmeklambri kruvi","Juhtmeklambri kruvi","Juhtmeklambri kruvi"]
["","Kasutusjuhend","","","","Kasutusjuhend","Kasutusjuhend","Kasutusjuhend","Kasutusjuhend","Kasutusjuhend","Kasutusjuhend","Kasutusjuhend"]
["","Klambri metall","","","","Klambri metall","Klambri metall","Klambri metall","Klambri metall","Klambri metall","Klambri metall","Klambri metall"]
["","Klambrid","","","","Klambrid","Klambrid","Klambrid","Klambrid","Klambrid","Klambrid","Klambrid"]
["","Vastavusdeklaratsioon","","","","Vastavusdeklaratsioon","Vastavusdeklaratsioon","Vastavusdeklaratsioon","Vastavusdeklaratsioon","Vastavusdeklaratsioon","Vastavusdeklaratsioon","Vastavusdeklaratsioon"]
["","Tühjendusvoolik","","","","Tühjendusvoolik","Tühjendusvoolik","Tühjendusvoolik","Tühjendusvoolik","Tühjendusvoolik","Tühjendusvoolik","Tühjendusvoolik"]
["","Paigaldusšabloon","","","","Paigaldusšabloon","Paigaldusšabloon","Paigaldusšabloon","Paigaldusšabloon","Paigaldusšabloon","Paigaldusšabloon","Paigaldusšabloon"]
["","Tihendusmaterjal","","","","Tihendusmaterjal","Tihendusmaterjal","Tihendusmaterjal","Tihendusmaterjal","Tihendusmaterjal","Tihendusmaterjal","Tihendusmaterjal"]
["Elektritoide","Nimetus","","","","VE","VE","VE","VE","VE","VE","VE"]
["","Faas","","","","1~","1~","1~","1~","1~","1~","1~"]
["","Sagedus","","","Hz","50/60","50/60","50/60","50/60","50/60","50/60","50/60"]
["","Pinge","","","V","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220"]