{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":5,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FLXS-B9 / RXS-L"]
[]
[]
[]
[]
["","","","","FLXS35BAVMB9 / RXS35L2V1B"]
["Jahutusvõimsus","Min","","kW","1.2"]
["","Max","","kW","3.8"]
["","Nom","","kW","3.5"]
["Piping connections","Vedelik","Välisdiameeter","mm","6.35"]
["","Gaas","Välisdiameeter","mm","9.5"]
["","Drain","OD","mm","18.0"]
["Nominaalne kasutegur","Aastane energiatarve","","kWh","565"]
["","Energiatõhususe suhtarv","","","3.10"]
["","COP","","","3.57"]
["","Energiamärgistamise direktiiv","Jahutus","","B"]
["","","Küte","","B"]
["Küttevõimsus","Nom","","kW","4.0"]
["","Min","","kW","1.4"]
["","Max","","kW","5.0"]
["Märkused","","","","(1) - EER/COP vastavalt Eurovent 2012-le, kasutamiseks ainult väljaspool EL-i"]
["","","","","(2) - 220V"]
["","","","","(3) - 230 V"]
["","","","","(4) - 240V"]
["","","","","(5) - Jahutus: sisetemp. 27 °CDB, 19,0 °CWB; välistemp. 35 °CDB, 24 °CWB; ekvivalentne torustiku pikkus: 5 m"]
["","","","","(6) - Küte: sisetemp. 20 °CDB; välistemp. 7 °CDB, 6 °CWB; ekvivalentne jahutustorustik: 5 m"]
["","","","","(7) - Nimikasutegur: jahutus 35°/27° nominaalkoormusel, küte 7°/20° nominaalkoormusel"]