{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":44,"n_cols":5,"rows_kept":44,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FLXS-B9"]
[]
[]
[]
[]
["","","","","FLXS35BAVMB9"]
["Mürarõhutase","Küte","kiire","dBA","46"]
["","","Vaikne töö","dBA","30"]
["","","aeglane","dBA","33"]
["","Jahutus","Vaikne töö","dBA","29"]
["","","aeglane","dBA","32"]
["","","kiire","dBA","38"]
["","","Nom","dBA","36"]
["","Jahutus","Nom","dBA","35"]
["Standardsed lisatarvikud","Paigaldusjuhend","","","1"]
["","Kasutusjuhend","","","1"]
["","Infrapunaühendusega kaugjuhtimispult","","","1"]
["","AAA kuivelement patareid","","","2"]
["","Kaugjuhtimispuldi hoidik","","","1"]
["","Paigaldusplaat","","","1"]
["","Torustiku soojusisolatsioon (jahutustoru)","","","8"]
["","Õhupuhastusfilter","","","1"]
["","Fotokatalüüsi lõhnafilter","","","1"]
["","Külgkaas","","","2"]
["","Kinnitusriba","","","4"]
["Control systems","Infrared remote control","","","ARC433B67"]
["Toruühendused","Vedelik","Välisdiameeter","mm","6.35"]
["","Gaas","Välisdiameeter","mm","9.5"]
["","Drain","","","18"]
["Sound power level","Jahutamine","","dBA","53"]
["","Soojendamine","","dBA","59"]
["Mõõtmed","Ühik","Laius","mm","1,050"]
["","","Sügavus","mm","200"]
["","","Kõrgus","mm","490"]
["Casing","Colour","","","Mandlivalge"]
["Kaal","Ühik","","kg","16"]
["Power supply","Phase","","","1~"]
["","Sagedus","","Hz","50"]
["","Nimetus","","","VM"]
["","Pinge","","V","220-240"]
["Märkused","","","","(1) - 220V"]
["","","","","(2) - 230 V"]
["","","","","(3) - 240V"]
["","","","","(4) - Multi-süsteemi välisseadmega ühendamisel vaadake multi-süsteemi välisseadme tehnilisi andmeid."]