{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":9,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FNA-A9"]
[]
[]
[]
[]
["","","","","","FNA25A2VEB9","FNA35A2VEB9","FNA50A2VEB9","FNA60A2VEB9"]
["Mürarõhutase","Küte","","kiire","dBA","33.0","33.0","36.0","36.0"]
["","","","Nom","dBA","31.0","31.0","33.0","33.0"]
["","","","aeglane","dBA","28.0","28.0","30.0","30.0"]
["","Jahutus","","Keskmine","dBA","31.0","31.0","33.0","33.0"]
["","","","aeglane","dBA","28.0","28.0","30.0","30.0"]
["","","","kiire","dBA","33.0","33.0","36.0","36.0"]
["Juhtsüsteemid","Juhtmega kaugjuhtimine","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["","Infrared remote control","","","","BRC4C65","BRC4C65","BRC4C65","BRC4C65"]
["Piping connections","Vedelik","","Välisdiameeter","mm","6.35","6.35","6.35","6.35"]
["","Gaas","","Välisdiameeter","mm","9.52","9.52","12.7","12.7"]
["","Drain","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Müratase","Jahutamine","","","dBA","53.0","53.0","56.0","56.0"]
["Mõõtmed","Seade","","Laius","mm","790","790","1,190","1,190"]
["","","","Sügavus","mm","200","200","200","200"]
["","","","Kõrgus","mm","620, 720 (1)","620, 720 (1)","620, 720 (1)","620, 720 (1)"]
["Korpus","Materjal","","","","Galvaanitud teraplaat","Galvaanitud teraplaat","Galvaanitud teraplaat","Galvaanitud teraplaat"]
["","Colour","","","","Värvimata","Värvimata","Värvimata","Värvimata"]
["Kaal","Ühik","","","kg","23.0","23.0","30.0","30.0"]
["Ventilaator","Väline staatiline rõhk","","Kõrge","Pa","48","48","49","49"]
["","","","Nom.","Pa","30","30","40","40"]
["","Õhu vooluhulk","Küte","kiire","m³/min","8.7","8.7","16.0","16.0"]
["","","","aeglane","m³/min","7.3","7.3","13.5","13.5"]
["","","","Nom","m³/min","8.0","8.0","14.8","14.8"]
["","","Jahutus","aeglane","m³/min","7.3","7.3","13.5","13.5"]
["","","","Nom","m³/min","8.0","8.0","14.8","14.8"]
["","","","kiire","m³/min","8.7","8.7","16.0","16.0"]
["Power supply","Faas","","","","1~","1~","1~","1~"]
["","Nimetus","","","","VE","VE","VE","VE"]
["","Sagedus","","","Hz","50/60","50/60","50/60","50/60"]
["","Pinge","","","V","220-240/220","220-240/220","220-240/220","220-240/220"]
["Märkused","","","","","(1) - Sisaldab paigaldusjalgu","(1) - Sisaldab paigaldusjalgu","(1) - Sisaldab paigaldusjalgu","(1) - Sisaldab paigaldusjalgu"]
["","","","","","(2) - Müravõimsus on vastab müraallika poolt tekitatud müra \"võimsuse\" absoluutväärtusele.","(2) - Müravõimsus on vastab müraallika poolt tekitatud müra \"võimsuse\" absoluutväärtusele.","(2) - Müravõimsus on vastab müraallika poolt tekitatud müra \"võimsuse\" absoluutväärtusele.","(2) - Müravõimsus on vastab müraallika poolt tekitatud müra \"võimsuse\" absoluutväärtusele."]