{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":6,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXA-BB / RXA-B8"]
[]
[]
[]
[]
["","","","","FTXA42B2V1BB / RXA42B5V1B8","FTXA50B2V1BB / RXA50B5V1B8"]
["Jahutusvõimsus","Min","","kW","1.7","1.7"]
["","Nom","","kW","4.2","5"]
["","Max","","kW","5","5.3"]
["Küttevõimsus","Min","","kW","1.7","1.7"]
["","Nom","","kW","5.4","5.8"]
["","Max","","kW","6","6.5"]
["Nimikasutegur","Energiatõhususe suhtarv","","","3.99","3.68"]
["","COP","","","4.12","4"]
["","Aastane energiatarve","","kWh","526","679"]
["Nominaalne kasutegur","Energiamärgistamise direktiiv","Jahutus","","A","A"]
["","","Küte","","A","A"]
["Ruumide jahutus","Energiatõhususe klass","","","A++","A++"]
["","Võimsus","Pdesign","kW","4.2","5"]
["","SEER","","","7.5","7.33"]
["","Aastane energiatarbimine","","kWh/a","196","239"]
["Ruumide küte (keskmine kliima)","Energiatõhususe klass","","","A++","A++"]
["","Võimsus","Pdesign","kW","3.8","4"]
["","SCOP/A","","","4.6","4.6"]
["","Pdh küttevõimsus temperatuuril -10°","","kW","3.04","3.19"]
["","Aastane energiatarbimine","","kWh/a","1,156","1,218"]
["Märkused","","","","(1) - Jahutuse nim. põhinevad: sisetemp.: 27 °CDB, 19 °CWB, välistemp.: 35 °CDB, samaväärne külmaaine torustik: 5m, kõrguste vahe: 0 m","(1) - Jahutuse nim. põhinevad: sisetemp.: 27 °CDB, 19 °CWB, välistemp.: 35 °CDB, samaväärne külmaaine torustik: 5m, kõrguste vahe: 0 m"]
["","","","","(2) - Tavaliste küttevõimsuste kehtivuse tingimused: sisetemperatuur: 20 °CDB, välistemperatuur: 7 °CDB, 6 °CWB, ekvivalentne jahutustorustik: 5 m, kõrguste vahe: 0 m.","(2) - Tavaliste küttevõimsuste kehtivuse tingimused: sisetemperatuur: 20 °CDB, välistemperatuur: 7 °CDB, 6 °CWB, ekvivalentne jahutustorustik: 5 m, kõrguste vahe: 0 m."]
["","","","","(3) - Vt töövahemiku kohta eraldi joonist","(3) - Vt töövahemiku kohta eraldi joonist"]