{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":10,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXA-BS"]
[]
[]
[]
[]
["","","","","","FTXA20B2V1BS","FTXA25B2V1BS","FTXA35B2V1BS","FTXA42B2V1BS","FTXA50B2V1BS"]
["Sisendvõimsus","Jahutus","","Nom","kW","0.02","0.022","0.023","0.028","0.030"]
["","Küte","","Nom","kW","0.02","0.02","0.022","0.036","0.039"]
["Korpus","Värvus","","","","Hõbedane","Hõbedane","Hõbedane","Hõbedane","Hõbedane"]
["Mõõtmed","Ühik","","Kõrgus","mm","295","295","295","295","295"]
["","","","Laius","mm","798","798","798","798","798"]
["","","","Sügavus","mm","189","189","189","189","189"]
["Kaal","Ühik","","","kg","11.5","11.5","11.5","11.5","11.5"]
["Ventilaator","Õhu vooluhulk","Jahutus","kiire","m³/min","11","11.5","11.9","13.1","13.5"]
["","Õhuvoolu kiirus","Jahutus","Keskmine","m³/min","8.2","8.6","8.6","9.8","10.4"]
["","","","aeglane","m³/min","6.1","6.1","6.1","7.2","7.6"]
["","","","Vaikne töö","m³/min","4.6","4.6","4.6","4.6","5.2"]
["","","Küte","kiire","m³/min","10.9","11.1","11.5","14.6","15.1"]
["","Õhuvoolu kiirus","Küte","Keskmine","m³/min","8.7","9","9","10.5","11.1"]
["","","Küte","aeglane","m³/min","6.4","6.4","6.4","7.7","8.2"]
["","","","Vaikne töö","m³/min","4.5","4.5","4.5","5.2","5.7"]
["Helivõimsustase","Jahutamine","","","dBA","57","57","60","60","60"]
["Mürarõhutase","Jahutus","","kiire","dBA","39","40","41","45","46"]
["Helirõhu tase","Jahutus","","Keskmine","dBA","32","33","33","37","39"]
["Mürarõhutase","Jahutus","","aeglane","dBA","25","25","25","29","31"]
["","","","Vaikne töö","dBA","19","19","19","21","24"]
["","Küte","","kiire","dBA","39","40","41","45","46"]
["Helirõhu tase","Küte","","Keskmine","dBA","32","33","33","37","42"]
["Mürarõhutase","Küte","","aeglane","dBA","25","25","25","29","33"]
["","","","Vaikne töö","dBA","19","19","19","21","24"]
["Külmaaine","GWP","","","","675","675","675","675","675.0"]
["Toruühendused","Vedelik","","Välisdiameeter","mm","6.35","6.35","6.35","6.35","6.35"]
["","Gaas","","Välisdiameeter","mm","9.5","9.5","9.5","12.7","12.70"]
["","Tühjendus","","","","18","18","18","18","18"]
["Juhtsüsteemid","Infrapunakaugjuhtimine","","","","ARC466A58","ARC466A58","ARC466A58","ARC466A58","ARC466A58"]
["","Juhtmega kaugjuhtimine","","","","BRC073","BRC073","BRC073","BRC073","BRC073"]
["Standardsed lisatarvikud","Installation manual","","","","1","1","1","1","1"]
["","Screw cover","","","","2","2","2","2","2"]
["","AAA dry-cell batteries","","","","2","2","2","2","2"]
["","General safety precautions","","","","1","1","1","1","1"]
["","Operation manual","","","","1","1","1","1","1"]
["","Air filter","","","","2","2","2","2","2"]
["","Infrared remote control","","","","1","1","1","1","1"]
["","Remote controller mounting plate","","","","1","1","1","1","1"]
["","Screw bag","","","","1","1","1","1","1"]
["Elektritoide","Nimetus","","","","V1","V1","V1","V1","V1"]
["","Faas","","","","1~","1~","1~","1~","1~"]
["","Sagedus","","","Hz","50","50","50","50","50"]
["","Pinge","","","V","220-240","220-240","220-240","220-240","220-240"]