{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":6,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXG-LW / RXLG-M"]
[]
[]
[]
[]
["","","","","FTXG25LV1BW / RXLG25M2V1B","FTXG35LV1BW / RXLG35M2V1B"]
["Outdoor unit","","","","RXLG25M","RXLG35M"]
["Jahutusvõimsus","Min","","kW","1.3","1.4"]
["","Nom","","kW","2.5","3.5"]
["","Max","","kW","4.0","4.6"]
["Küttevõimsus","Min","","kW","1.0","1.0"]
["","Nom","","kW","4.4","5.1"]
["","Max","","kW","6.1, 3.6","6.7, 4.2"]
["Nimikasutegur","Energiatõhususe suhtarv","","","3.68","3.57"]
["","COP","","","4.31","3.89"]
["","Aastane energiatarve","","kWh","340","490"]
["Nominaalne kasutegur","Energiamärgistamise direktiiv","Jahutus","","A","A"]
["","","Küte","","A","A"]
["Torustikuühendused","Tühjendus","OD","mm","18","18"]
["Toruühendused","Gaas","Välisdiameeter","mm","9.5","9.5"]
["","Vedelik","Välisdiameeter","mm","6.35","6.35"]
["Ruumide jahutus","Energiatõhususe klass","","","A++","A++"]
["","Võimsus","Pdesign","kW","2.50","3.50"]
["","SEER","","","7.04","6.67"]
["","Aastane energiatarbimine","","kWh/a","124","184"]
["Ruumide küte (keskmine kliima)","Energiatõhususe klass","","","A++","A++"]
["","Võimsus","Pdesign","kW","2.50","3.00"]
["","SCOP/A","","","4.64","4.60"]
["","Aastane energiatarbimine","","kWh/a","755","913"]
["Märkused","","","","(1) - EER/COP vastavalt Eurovent 2012-le, kasutamiseks ainult väljaspool EL-i","(1) - EER/COP vastavalt Eurovent 2012-le, kasutamiseks ainult väljaspool EL-i"]
["","","","","(2) - Nimikasutegur: jahutus 35°/27° nominaalkoormusel, küte 7°/20° nominaalkoormusel","(2) - Nimikasutegur: jahutus 35°/27° nominaalkoormusel, küte 7°/20° nominaalkoormusel"]
["","","","","(3) - 220V","(3) - 220V"]
["","","","","(4) - 230 V","(4) - 230 V"]
["","","","","(5) - 240V","(5) - 240V"]
["","","","","(6) - Minimaalse nimikütteväärtuse jaoks on sisepaigaldise ventilaator seadistatud astmele SL","(6) - Minimaalse nimikütteväärtuse jaoks on sisepaigaldise ventilaator seadistatud astmele SL"]
["","","","","(7) - Maksimaalne küttevõimsus -15°C välistemperatuuri juures","(7) - Maksimaalne küttevõimsus -15°C välistemperatuuri juures"]