{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":6,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXL-JV / RXL-M"]
[]
[]
[]
[]
["","","","","FTXL25J2V1B / RXL25M2V1B","FTXL35J2V1B / RXL35M2V1B"]
["Jahutusvõimsus","Min","","kW","1.2","1.3"]
["","Max","","kW","3.4","3.8"]
["Toruühendused","Vedelik","Välisdiameeter","mm","6.35","6.35"]
["","Gaas","Välisdiameeter","mm","9.5","9.5"]
["","Drain","OD","mm","18","18"]
["Nominaalne kasutegur","Aastane energiatarve","","kWh","400.5","570"]
["","Energiatõhususe suhtarv","","","3.12","3.07"]
["","COP","","","4.43","4.21"]
["","Energiamärgistamise direktiiv","Jahutus","","B","B"]
["","","Küte","","A","A"]
["Küttevõimsus","Min","","kW","1.1","1.2"]
["","Max","","kW","5.5","6.0"]
["Märkused","","","","(1) - Minimaalse nimikütteväärtuse jaoks on sisepaigaldise ventilaator seadistatud astmele SL","(1) - Minimaalse nimikütteväärtuse jaoks on sisepaigaldise ventilaator seadistatud astmele SL"]
["","","","","(2) - 220V","(2) - 220V"]
["","","","","(3) - 230 V","(3) - 230 V"]
["","","","","(4) - 240V","(4) - 240V"]
["","","","","(5) - EER/COP vastavalt Eurovent 2012-le, kasutamiseks ainult väljaspool EL-i","(5) - EER/COP vastavalt Eurovent 2012-le, kasutamiseks ainult väljaspool EL-i"]
["","","","","(6) - Nimikasutegur: jahutus 35°/27° nominaalkoormusel, küte 7°/20° nominaalkoormusel","(6) - Nimikasutegur: jahutus 35°/27° nominaalkoormusel, küte 7°/20° nominaalkoormusel"]