{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":6,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXP-M9 / 2MXM-A"]
[]
[]
[]
[]
["","","","","FTXP20M5V1B9 / FTXP20M5V1B9 / 2MXM40A2V1B","FTXP20M5V1B9 / FTXP20M5V1B9 / 2MXM50A2V1B"]
["Jahutusvõimsus","Nom","","kW","4.00"]
["Küttevõimsus","Nom","","kW","4.20"]
["Nimikasutegur","Energiatõhususe suhtarv","","","3.71"]
["","COP","","","3.75"]
["","Aastane energiatarve","","kWh","539"]
["Nominaalne kasutegur","Energiamärgistamise direktiiv","Jahutus","","A"]
["","","Küte","","A"]
["Ruumide jahutus","Energiatõhususe klass","","","A++"]
["","Võimsus","Pdesign","kW","4.00"]
["","SEER","","","7.74"]
["","Aastane energiatarbimine","","kWh/a","181"]
["Ruumide küte (keskmine kliima)","Energiatõhususe klass","","","A+"]
["","Võimsus","Pdesign","kW","3.20"]
["","SCOP/A","","","4.30"]
["","Pdh küttevõimsus temperatuuril -10°","","kW","2.46"]
["","Aastane energiatarbimine","","kWh/a","1041"]
["Energiatõhususe klass","","","","A+++ ~ D"]
["Märkused","","","","(1) - Jahutuse nim. põhinevad: sisetemp.: 27 °CDB, 19 °CWB, välistemp.: 35 °CDB, samaväärne külmaaine torustik: 5m, kõrguste vahe: 0 m","(1) - Jahutuse nimivõimsused põhinevad: sisetemp.: 27 °CDB, 19 °CWB, välistemp.: 35 °CDB, samaväärne külmaaine torustik: 5m, kõrguste vahe: 0 m"]
["","","","","(2) - Tavaliste küttevõimsuste kehtivuse tingimused: sisetemperatuur: 20 °CDB, välistemperatuur: 7 °CDB, 6 °CWB, ekvivalentne jahutustorustik: 5 m, kõrguste vahe: 0 m.","(2) - Tavaliste küttevõimsuste kehtivuse tingimused: sisetemperatuur: 20 °CDB, välistemperatuur: 7 °CDB, 6 °CWB, ekvivalentne jahutustorustik: 5 m, kõrguste vahe: 0 m."]
["","","","","(3) - Vt töövahemiku kohta eraldi joonist","(3) - Vt töövahemiku kohta eraldi joonist"]
["","","","","(4) - Vt eraldi elektriandmete joonist","(4) - Vt eraldi elektriandmete joonist"]
["Jahutusvõimsus","Nom","","kW","","4.00"]
["Küttevõimsus","Nom","","kW","","5.20"]
["Nominaalne kasutegur","Aastane energiatarve","","kWh","","554"]
["","COP","","","","3.68"]
["","Energiatõhususe suhtarv","","","","3.61"]
["","Energiamärgistamise direktiiv","Jahutus","","","A"]
["","","Küte","","","A"]