{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":48,"n_cols":8,"rows_kept":48,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXP-M9"]
[]
[]
[]
[]
["","","","","","FTXP20M5V1B9","FTXP25M5V1B9","FTXP35M5V1B9"]
["Sisendvõimsus","Jahutus","","Nom","kW","0.019","0.02","0.032"]
["","Küte","","Nom","kW","0.023","0.023","0.032"]
["Korpus","Värvus","","","","Valge","Valge","Valge"]
["Mõõtmed","Ühik","","Kõrgus","mm","286","286","286"]
["","","","Laius","mm","770","770","770"]
["","","","Sügavus","mm","225","225","225"]
["Kaal","Ühik","","","kg","8.5","8.5","9"]
["Ventilaator","Õhu vooluhulk","Jahutus","kiire","m³/min","9.5","9.7","11.5"]
["","Õhuvoolu kiirus","Jahutus","Keskmine","m³/min","7.4","7.7","8.3"]
["","","","aeglane","m³/min","5.6","5.8","6.3"]
["","","","Vaikne töö","m³/min","4.2","4.2","4.5"]
["","","Küte","kiire","m³/min","10.4","10.4","11.5"]
["","Õhuvoolu kiirus","Küte","Keskmine","m³/min","8.1","8.1","9"]
["","","Küte","aeglane","m³/min","6.2","6.4","7"]
["","","","Vaikne töö","m³/min","5.2","5.2","5.3"]
["Helivõimsustase","Jahutamine","","","dBA","55","55","58"]
["","Soojendamine","","","dBA","55","55","58"]
["Mürarõhutase","Jahutus","","kiire","dBA","39","40","43"]
["Helirõhu tase","Jahutus","","Keskmine","dBA","33","33","34"]
["Mürarõhutase","Jahutus","","aeglane","dBA","25","26","27"]
["","","","Vaikne töö","dBA","19","19","20"]
["","Küte","","kiire","dBA","39","40","40"]
["Helirõhu tase","Küte","","Keskmine","dBA","34","34","35"]
["Mürarõhutase","Küte","","aeglane","dBA","28","28","29"]
["","","","Vaikne töö","dBA","21","21","21"]
["Toruühendused","Vedelik","","Välisdiameeter","mm","6.35","6.35","6.35"]
["","Gaas","","Välisdiameeter","mm","9.5","9.5","9.5"]
["","Tühjendus","","","","18","18","18"]
["Juhtimissüsteemid","Infrared remote control","","","","ARC480A53","ARC480A53","ARC480A53"]
["Juhtsüsteemid","Juhtmega kaugjuhtimine","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["Standardsed lisatarvikud","Installation manual","","","","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2"]
["","Operation manual","","","","1","1","1"]
["","Titanium apatite deodorizing filter","","","","1","2","2"]
["","Silver particle filter","","","","1"]
["","Indoor unit fixing screws","","","","2","2","2"]
["","Infrared remote control","","","","1","1","1"]
["","Mounting plate","","","","1","1","1"]
["","Remote control holder","","","","1","1","1"]
["Elektritoide","Faas","","","","1~","1~","1~"]
["","Sagedus","","","Hz","50","50","50"]
["","Pinge","","","V","220-240","220-240","220-240"]