{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":6,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXS-F / RXS-F"]
[]
[]
[]
[]
["","","","","FTXS60FV1B / RXS60F2V1B","FTXS71FV1B / RXS71FV1B"]
["Jahutusvõimsus","Min","","kW","1.7","2.3"]
["","Max","","kW","6.7","8.5"]
["","Nom","","kW","6.0 (1)","7.1 (1)"]
["Toruühendused","Vedelik","Välisdiameeter","mm","6.35","6.35"]
["","Gaas","Välisdiameeter","mm","12.7","15.9"]
["","Drain","OD","mm","18.0","18.0"]
["Nominaalne kasutegur","Aastane energiatarve","","kWh","995","1,175"]
["","Energiatõhususe suhtarv","","","3.02","3.02"]
["","COP","","","3.43","3.22"]
["","Energiamärgistamise direktiiv","Jahutus","","B","B"]
["","","Küte","","B","C"]
["Küttevõimsus","Nom","","kW","7.0 (2)","8.2 (2)"]
["","Min","","kW","1.7","2.3"]
["","Max","","kW","8.0","10.2"]
["Märkused","","","","(1) - Jahutus: sisetemp. 27 °CDB, 19 °CWB; välistemp. 35 °CDB, 24 °CWB; ekvivalentne torustiku pikkus: 7,5 m","(1) - Jahutus: sisetemp. 27 °CDB, 19 °CWB; välistemp. 35 °CDB, 24 °CWB; ekvivalentne torustiku pikkus: 7,5 m"]
["","","","","(2) - Küte: sisetemp. 20 °CDB; välistemp. 7 °CDB, 6 °CWB; ekvivalentne jahutustorustik: 7,5 m","(2) - Küte: sisetemp. 20 °CDB; välistemp. 7 °CDB, 6 °CWB; ekvivalentne jahutustorustik: 7,5 m"]
["","","","","(3) - Nimikasutegur: jahutus 35°/27° nominaalkoormusel, küte 7°/20° nominaalkoormusel","(3) - Nimikasutegur: jahutus 35°/27° nominaalkoormusel, küte 7°/20° nominaalkoormusel"]