{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":85,"n_cols":12,"rows_kept":85,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXS-G"]
[]
[]
[]
[]
["","","","","","FTXS20G2V1B","FTXS25G2V1B","FTXS35G2V1B","FTXS42G2V1B","FTXS50G2V1B","FTXS60GV1B","FTXS71GV1B"]
["Mürarõhutase","Küte","","kiire","dBA","38","39","42","42","44","","46"]
["","","","Vaikne töö","dBA","25","25","26","30","31","","34"]
["","","","aeglane","dBA","28","28","29","33","34","","37"]
["","Jahutus","","Vaikne töö","dBA","22","22","23","30","31","","34"]
["","","","aeglane","dBA","25","25","26","33","34","","37"]
["","","","kiire","dBA","38","38","42","42","43","","46"]
["","","","Nom","dBA","33","34","36","38","39","","42"]
["","Jahutus","","Nom","dBA","32","32","34","38","39","","42"]
["Standardsed lisatarvikud","Titaanapatiidist fotokatalüütiline õhupuhastusfilter","","","","2","2","2","2","2"]
["","Kasutusjuhend","","","","1","1","1","1","1","","1"]
["","Paigaldusjuhend","","","","1","1","1","1","1","","1"]
["","Traadita juhtimispult","","","","1","1","1","1","1","","1"]
["","Akud","","","","2","2","2","2","2","","2"]
["","Kaugjuhtimispuldi hoidik","","","","1","1","1","1","1","","1"]
["","Siseseadme kinnituskruvid","","","","2","2","2","2","2","","2"]
["","Paigaldusplaat","","","","1","1","1","1","1","","1"]
["Juhtsüsteemid","Infrared remote control","","","","","","","","","","ARC452A3"]
["Toruühendused","Vedelik","","Välisdiameeter","mm","6.35","6.35","6.35","6.35","6.35","","6.35"]
["","Gaas","","Välisdiameeter","mm","9.52","9.52","9.52","9.52","12.70","","15.9"]
["","Tühjendus","","","","18","18","18","18","18","","18"]
["Sisendvõimsus","Jahutus","","Nom","kW","","","","","","","0.045 (2), 0.045 (3), 0.045 (4)"]
["","Küte","","Nom","kW","","","","","","","0.060 (2), 0.060 (3), 0.060 (4)"]
["Sound power level","Jahutamine","","","dBA","54","54","58","58","59","","63"]
["","Soojendamine","","","dBA","54","55","58","58","60","","62"]
["Mõõtmed","Ühik","","Laius","mm","800","800","800","800","800","","1,050"]
["","","","Sügavus","mm","215","215","215","215","215","","250"]
["","","","Kõrgus","mm","295","295","295","295","295","","290"]
["Korpus","Värvus","","","","Valge","Valge","Valge","Valge","Valge","","Valge"]
["Kaal","Ühik","","","kg","9","9","10","10","10","","12"]
["Power supply","Faas","","","","1~","1~","1~","1~","1~","","1~"]
["","Sagedus","","","Hz","50","50","50","50","50","","50"]
["","Nimetus","","","","V1","V1","V1","V1","V1","","V1"]
["","Pinge","","","V","220-240","220-240","220-240","220-240","220-240","","220-240"]
["Märkused","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - SL: Õhuvoo seade, mis tagab ventilaatori vaikse töö"]
["","","","","","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 220V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 230 V"]
["Ventilaator","Õhu vooluhulk","Jahutus","Nom","m³/min","","","","","","16.0"]
["Mürarõhutase","Jahutus","","Nom","dBA","","","","","","41"]
["Ventilaator","Õhu vooluhulk","Küte","Nom","m³/min","","","","","","14.9"]
["Mürarõhutase","Küte","","Nom","dBA","","","","","","40"]
["Sisendvõimsus","Jahutus","","Nom","kW","","","","","","0.040 (4) (2) (3), 0.040 (4) (2) (3), 0.040 (4) (2) (3)"]
["","Küte","","Nom","kW","","","","","","0.045 (4) (2) (3), 0.045 (4) (2) (3), 0.045 (4) (2) (3)"]
["Korpus","Värvus","","","","","","","","","Valge"]
["Mõõtmed","Ühik","","Kõrgus","mm","","","","","","290"]
["","","","Laius","mm","","","","","","1050"]
["","","","Sügavus","mm","","","","","","250"]
["Kaal","Ühik","","","kg","","","","","","12"]
["Ventilaator","Õhu vooluhulk","Jahutus","kiire","m³/min","","","","","","16.0"]
["","","","aeglane","m³/min","","","","","","11.3"]
["","","","Vaikne töö","m³/min","","","","","","10.1"]
["","","Küte","kiire","m³/min","","","","","","17.2"]
["","","","aeglane","m³/min","","","","","","12.6"]
["","","","Vaikne töö","m³/min","","","","","","11.3"]
["Helivõimsustase","Jahutamine","","","dBA","","","","","","60"]
["","Soojendamine","","","dBA","","","","","","59"]
["Mürarõhutase","Jahutus","","kiire","dBA","","","","","","45"]
["","","","aeglane","dBA","","","","","","36"]
["","","","Vaikne töö","dBA","","","","","","33"]
["","Küte","","kiire","dBA","","","","","","44"]
["","","","aeglane","dBA","","","","","","35"]
["","","","Vaikne töö","dBA","","","","","","32"]
["Toruühendused","Vedelik","","Välisdiameeter","mm","","","","","","6.35"]
["","Gaas","","Välisdiameeter","mm","","","","","","12.7"]
["","Tühjendus","","","","","","","","","18"]
["Juhtsüsteemid","Infrapunakaugjuhtimine","","","","","","","","","ARC452A3"]
["Standardsed lisatarvikud","Installation manual","","","","","","","","","1"]
["","Wireless remote control","","","","","","","","","1"]
["","Operation manual","","","","","","","","","1"]
["","Batteries","","","","","","","","","2"]
["","Indoor unit fixing screws","","","","","","","","","2"]
["","Mounting plate","","","","","","","","","1"]
["","Remote control holder","","","","","","","","","1"]
["","Titanium apatite photocatalytic air purification filter","","","","","","","","","2"]
["Elektritoide","Nimetus","","","","","","","","","V1"]
["","Faas","","","","","","","","","1~"]
["","Sagedus","","","Hz","","","","","","50"]
["","Pinge","","","V","","","","","","220-240"]
["Standardsed lisatarvikud","Titaanapatiidist fotokatalüütiline õhupuhastusfilter ilma raamita","","","","","","","","","","2"]
["Märkused","","","","","","","","","","","(4) - 240V"]