{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":5,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTA-AW"]
[]
[]
[]
[]
["","","","","FTXTA30A2V1BW"]
["Helirõhu tase","Küte","kiire","dBA","41"]
["","","Keskmine","dBA","31"]
["","","Vaikne töö","dBA","19"]
["","","aeglane","dBA","24"]
["","Jahutus","Keskmine","dBA","32"]
["","","Vaikne töö","dBA","20"]
["","","aeglane","dBA","25"]
["","","kiire","dBA","43"]
["Standardsed lisatarvikud","Paigaldusjuhend","","","1"]
["","Kasutusjuhend","","","1"]
["","Õhufilter","","","2"]
["","Infrapunaühendusega kaugjuhtimispult","","","1"]
["","Kaugjuhtimispuldi paigaldusplaat","","","1"]
["","Kruvide kott","","","1"]
["","Kruvide kaas","","","2"]
["","AAA kuivelement patareid","","","2"]
["","Üldised ohutusmeetmed","","","1"]
["Jahutusaine","GWP","","","675.0"]
["Control systems","Wired remote control","","","BRC073A4"]
["","Infrared remote control","","","ARC466A59"]
["Toruühendused","Vedelik","Välisdiameeter","mm","6.35"]
["","Gaas","Välisdiameeter","mm","9.50"]
["","Tühjendus","","","18"]
["Sisendvõimsus","Jahutus","Nom","kW","0.023"]
["","Küte","Nom","kW","0.022"]
["Müratase","Jahutamine","","dBA","60"]
["","Soojendamine","","dBA","60"]
["Mõõtmed","Ühik","Laius","mm","798"]
["","","Sügavus","mm","189"]
["","","Kõrgus","mm","295"]
["Korpus","Colour","","","Valge"]
["Kaal","Ühik","","kg","11.5"]
["Power supply","Phase","","","1~"]
["","Sagedus","","Hz","50"]
["","Nimetus","","","V1"]
["","Pinge","","V","220-240"]