{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":55,"n_cols":7,"rows_kept":55,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTM-A"]
[]
[]
[]
[]
["","","","","","FTXTM30A2V1B","FTXTM40A2V1B"]
["Sisendvõimsus","Jahutus","","Nom","kW","0.029","0.053"]
["","Küte","","Nom","kW","0.024","0.06"]
["Korpus","Värvus","","","","Valge","Valge"]
["Mõõtmed","Ühik","","Kõrgus","mm","298","298"]
["","","","Laius","mm","804","997"]
["","","","Sügavus","mm","252","292"]
["Kaal","Ühik","","","kg","12","15"]
["Ventilaator","Õhu vooluhulk","Jahutus","kiire","m³/min","13.2","15.1"]
["","Õhuvoolu kiirus","Jahutus","Keskmine","m³/min","8.1","9.2"]
["","","","aeglane","m³/min","5.6","5.6"]
["","","","Vaikne töö","m³/min","4.8","4.8"]
["","","Küte","kiire","m³/min","11.7","17"]
["","Õhuvoolu kiirus","Küte","Keskmine","m³/min","7.7","10"]
["","","Küte","aeglane","m³/min","5.6","6"]
["","","","Vaikne töö","m³/min","4.7","5.1"]
["Helivõimsustase","Jahutamine","","","dBA","60","60"]
["","Soojendamine","","","dBA","59","60"]
["Mürarõhutase","Jahutus","","kiire","dBA","45","46"]
["Helirõhu tase","Jahutus","","Keskmine","dBA","33","32"]
["Mürarõhutase","Jahutus","","aeglane","dBA","25","24"]
["","","","Vaikne töö","dBA","21","20"]
["","Küte","","kiire","dBA","43","46"]
["Helirõhu tase","Küte","","Keskmine","dBA","31","31"]
["Mürarõhutase","Küte","","aeglane","dBA","22","22"]
["","","","Vaikne töö","dBA","19","19"]
["Külmaaine","GWP","","","","675","675"]
["Toruühendused","Vedelik","","Välisdiameeter","mm","6.35","6.35"]
["","Gaas","","Välisdiameeter","mm","9.5","9.5"]
["","Tühjendus","","","","18","18"]
["Juhtsüsteemid","Infrapunakaugjuhtimine","","","","ARC466A83","ARC466A83"]
["Standardsed lisatarvikud","FTXTM30A2V1B","","","","1"]
["","Installation manual","","","","1","1"]
["","Wireless remote control","","","","1","1"]
["","Screw cover","","","","2","2"]
["","AAA dry-cell batteries","","","","2","2"]
["","General safety precautions","","","","1","1"]
["","Operation manual","","","","1","1"]
["","Titanium apatite deodorizing filter","","","","1","1"]
["","Silver particle filter","","","","1","1"]
["","Remote control holder","","","","1","1"]
["","Screw bag","","","","1","1"]
["Elektritoide","Nimetus","","","","V1","V1"]
["","Faas","","","","1~","1~"]
["","Sagedus","","","Hz","50","50"]
["","Pinge","","","V","220-240","220-240"]
["Märkused","","","","","(1) - Jahutus: sisetemp. 27 °CDB, 19 °CWB; välistemp. 35 °CDB, 24 °CWB; ekvivalentne torustiku pikkus: 5 m","(1) - Jahutus: sisetemp. 27 °CDB, 19 °CWB; välistemp. 35 °CDB, 24 °CWB; ekvivalentne torustiku pikkus: 5 m"]
["","","","","","(2) - Küte: sisetemp. 20 °CDB; välistemp. 7 °CDB, 6 °CWB; ekvivalentne jahutustorustik: 5 m","(2) - Küte: sisetemp. 20 °CDB; välistemp. 7 °CDB, 6 °CWB; ekvivalentne jahutustorustik: 5 m"]
["","","","","","(3) - Vt eraldi elektriandmete joonist","(3) - Vt eraldi elektriandmete joonist"]
["Standardsed lisatarvikud","FTXTM40A2V1B","","","","","1"]