{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":94,"n_cols":7,"rows_kept":94,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTM-R"]
[]
[]
[]
[]
["","","","","","FTXTM30R2V1B","FTXTM40R2V1B"]
["Mürarõhutase","Küte","","kiire","dBA","45.0"]
["","","","Keskmine","dBA","31.0"]
["","","","Vaikne töö","dBA","19.0"]
["","","","aeglane","dBA","22.0"]
["","Jahutus","","Medium","dBA","33.0"]
["","","","Vaikne töö","dBA","21.0"]
["","","","aeglane","dBA","25.0"]
["","","","kiire","dBA","45.0"]
["Standardsed lisatarvikud","Paigaldusjuhend","","","","1"]
["","Kasutusjuhend","","","","1"]
["","Traadita juhtimispult","","","","1"]
["","AAA kuivelement patareid","","","","2"]
["","Kaugjuhtimispuldi hoidik","","","","1"]
["","Paigaldusplaat","","","","1"]
["","Siseseadme kinnituskruvid","","","","2"]
["","Hõbedaioonidega filter","","","","1"]
["Juhtsüsteemid","Wired remote control","","","","BRC073A1"]
["","Infrared remote control","","","","ARC466A75"]
["Piping connections","Vedelik","","Välisdiameeter","mm","6.35"]
["","Gaas","","Välisdiameeter","mm","9.50"]
["","Tühjendus","","","","18"]
["Sisendvõimsus","Jahutus","","Nom","kW","0.035"]
["","Küte","","Nom","kW","0.039"]
["Müratase","Jahutamine","","","dBA","60.0"]
["","Soojendamine","","","dBA","61.0"]
["Mõõtmed","Seade","","Laius","mm","778"]
["","","","Sügavus","mm","272"]
["","","","Kõrgus","mm","295"]
["Korpus","Colour","","","","Valge"]
["Kaal","Ühik","","","kg","10.0"]
["Ventilaator","Õhu vooluhulk","Küte","kiire","m³/min","12.5"]
["","","","aeglane","m³/min","4.9"]
["","","","Keskmine","m³/min","7.5"]
["","","","Vaikne töö","m³/min","4.0"]
["","","Jahutus","aeglane","m³/min","5.3"]
["","","","Keskmine","m³/min","7.8"]
["","","","kiire","m³/min","12.2"]
["","","","Vaikne töö","m³/min","4.1"]
["Power supply","Phase","","","","1~"]
["","Sagedus","","","Hz","50"]
["","Nimetus","","","","V1"]
["","Pinge","","","V","220-240"]
["Märkused","","","","","(1) - Jahutus: sisetemp. 27 °CDB, 19,0 °CWB; välistemp. 35 °CDB, 24 °CWB; ekvivalentne torustiku pikkus: 5 m"]
["","","","","","(2) - Küte: sisetemp. 20 °CDB; välistemp. 7 °CDB, 6 °CWB; ekvivalentne jahutustorustik: 5 m"]
["","","","","","(3) - Vt eraldi elektriandmete jooniseid"]
["Sisendvõimsus","Jahutus","","Nom","kW","","0.053"]
["","Küte","","Nom","kW","","0.06"]
["Korpus","Värvus","","","","","Valge"]
["Mõõtmed","Ühik","","Kõrgus","mm","","299"]
["","","","Laius","mm","","998"]
["","","","Sügavus","mm","","292"]
["Kaal","Ühik","","","kg","","14.5"]
["Ventilaator","Õhu vooluhulk","Jahutus","kiire","m³/min","","15.4"]
["","Õhuvoolu kiirus","Jahutus","Keskmine","m³/min","","9.5"]
["","","","aeglane","m³/min","","5.8"]
["","","","Vaikne töö","m³/min","","4.6"]
["","","Küte","kiire","m³/min","","17.5"]
["","Õhuvoolu kiirus","Küte","Keskmine","m³/min","","10.5"]
["","","Küte","aeglane","m³/min","","7.1"]
["","","","Vaikne töö","m³/min","","5.9"]
["Helivõimsustase","Jahutamine","","","dBA","","60"]
["","Soojendamine","","","dBA","","61"]
["Mürarõhutase","Jahutus","","kiire","dBA","","46"]
["Helirõhu tase","Jahutus","","Keskmine","dBA","","32"]
["Mürarõhutase","Jahutus","","aeglane","dBA","","24"]
["","","","Vaikne töö","dBA","","20"]
["","Küte","","kiire","dBA","","46"]
["Helirõhu tase","Küte","","Keskmine","dBA","","31"]
["Mürarõhutase","Küte","","aeglane","dBA","","22"]
["","","","Vaikne töö","dBA","","19"]
["Toruühendused","Vedelik","","Välisdiameeter","mm","","6.35"]
["","Gaas","","Välisdiameeter","mm","","9.5"]
["","Tühjendus","","","","","18"]
["Juhtsüsteemid","Infrared remote control","","","","","ARC466A75"]
["Juhtsüsteemid","Juhtmega kaugjuhtimine","","","","","BRC073A1"]
["Standardsed lisatarvikud","Installation manual","","","","","1"]
["","Wireless remote control","","","","","1"]
["","AAA dry-cell batteries","","","","","2"]
["","Operation manual","","","","","1"]
["","Titanium apatite deodorizing filter","","","","","1"]
["","Silver particle filter","","","","","1"]
["","Indoor unit fixing screws","","","","","2"]
["","Mounting plate","","","","","1"]
["","Remote control holder","","","","","1"]
["Elektritoide","Nimetus","","","","","V1"]
["","Faas","","","","","1~"]
["","Sagedus","","","Hz","","50"]
["","Pinge","","","V","","220-240"]