{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":6,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTP-A / RXTP-A"]
[]
[]
[]
[]
["","","","","FTXTP25A5V1B / RXTP25A2V1B","FTXTP35A5V1B / RXTP35A2V1B"]
["Jahutusvõimsus","Min","","kW","1","1"]
["","Nom","","kW","2.5","3.5"]
["","Max","","kW","4.1","4.5"]
["Küttevõimsus","Min","","kW","1","1"]
["","Nom","","kW","3.2","4"]
["","Max","","kW","6.2","6.7"]
["Nimikasutegur","Energiatõhususe suhtarv","","","4.88","4.71"]
["","COP","","","4.99","4.55"]
["","Aastane energiatarve","","kWh","256","372"]
["Nominaalne kasutegur","Energiamärgistamise direktiiv","Jahutus","","A","A"]
["","","Küte","","A","A"]
["Ruumide jahutus","Energiatõhususe klass","","","A+++","A+++"]
["","Võimsus","Pdesign","kW","2.5","3.5"]
["","SEER","","","8.55","8.55"]
["","Aastane energiatarbimine","","kWh/a","102","143"]
["Ruumide küte (keskmine kliima)","Energiatõhususe klass","","","A++","A++"]
["","Võimsus","Pdesign","kW","2.5","3"]
["","SCOP/A","","","4.95","4.85"]
["","Pdh küttevõimsus temperatuuril -10°","","kW","2.5","3"]
["","Aastane energiatarbimine","","kWh/a","707","866"]
["Märkused","","","","(1) - Tavaliste küttevõimsuste kehtivuse tingimused: sisetemperatuur: 20 °CDB, välistemperatuur: 7 °CDB, 6 °CWB, ekvivalentne jahutustorustik: 5 m, kõrguste vahe: 0 m.","(1) - Tavaliste küttevõimsuste kehtivuse tingimused: sisetemperatuur: 20 °CDB, välistemperatuur: 7 °CDB, 6 °CWB, ekvivalentne jahutustorustik: 5 m, kõrguste vahe: 0 m."]
["","","","","(2) - Jahutuse nim. põhinevad: sisetemp.: 27 °CDB, 19 °CWB, välistemp.: 35 °CDB, samaväärne külmaaine torustik: 5m, kõrguste vahe: 0 m","(2) - Jahutuse nim. põhinevad: sisetemp.: 27 °CDB, 19 °CWB, välistemp.: 35 °CDB, samaväärne külmaaine torustik: 5m, kõrguste vahe: 0 m"]
["","","","","(3) - Vt töövahemiku kohta eraldi joonist","(3) - Vt töövahemiku kohta eraldi joonist"]
["","","","","(4) - Vt eraldi elektriandmete joonist","(4) - Vt eraldi elektriandmete joonist"]