{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":55,"n_cols":7,"rows_kept":55,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTP-A"]
[]
[]
[]
[]
["","","","","","FTXTP25A5V1B","FTXTP35A5V1B"]
["Sisendvõimsus","Jahutus","","Nom","kW","0.032","0.032"]
["","Küte","","Nom","kW","0.032","0.032"]
["Korpus","Värvus","","","","Valge","Valge"]
["Mõõtmed","Ühik","","Kõrgus","mm","286","286"]
["","","","Laius","mm","770","770"]
["","","","Sügavus","mm","225","225"]
["Kaal","Ühik","","","kg","9","9"]
["Ventilaator","Õhu vooluhulk","Jahutus","kiire","m³/min","11","11"]
["","Õhuvoolu kiirus","Jahutus","Keskmine","m³/min","7.9","7.9"]
["","","","aeglane","m³/min","5","5"]
["","","","Vaikne töö","m³/min","3.7","3.7"]
["","","Küte","kiire","m³/min","10.5","10.5"]
["","Õhuvoolu kiirus","Küte","Keskmine","m³/min","9","9"]
["","","Küte","aeglane","m³/min","5.5","5.5"]
["","","","Vaikne töö","m³/min","4.4","4.4"]
["Helivõimsustase","Jahutamine","","","dBA","58","58"]
["","Soojendamine","","","dBA","58","58"]
["Mürarõhutase","Jahutus","","kiire","dBA","43","43"]
["Helirõhu tase","Jahutus","","Keskmine","dBA","35","35"]
["Mürarõhutase","Jahutus","","aeglane","dBA","26","26"]
["","","","Vaikne töö","dBA","21","21"]
["","Küte","","kiire","dBA","43","43"]
["Helirõhu tase","Küte","","Keskmine","dBA","35","35"]
["Mürarõhutase","Küte","","aeglane","dBA","26","26"]
["","","","Vaikne töö","dBA","21","21"]
["Külmaaine","GWP","","","","675","675"]
["Toruühendused","Vedelik","","Välisdiameeter","mm","6.35","6.35"]
["","Gaas","","Välisdiameeter","mm","9.5","9.5"]
["","Tühjendus","","","","18","18"]
["Juhtsüsteemid","Infrared remote control","","","","ARC480A78","ARC480A78"]
["Standardsed lisatarvikud","FTXTP25A5V1B","","","","1"]
["","Installation manual","","","","1","1"]
["","Wireless remote control","","","","1","1"]
["","Screw cover","","","","2","2"]
["","AAA dry-cell batteries","","","","2","2"]
["","General safety precautions","","","","1","1"]
["","Operation manual","","","","1","1"]
["","Titanium apatite deodorizing filter","","","","1","1"]
["","Silver particle filter","","","","1","1"]
["","Remote control holder","","","","1","1"]
["","Screw bag","","","","1","1"]
["Elektritoide","Nimetus","","","","V1","V1"]
["","Faas","","","","1~","1~"]
["","Sagedus","","","Hz","50","50"]
["","Pinge","","","V","220-240","220-240"]
["Märkused","","","","","(1) - Jahutus: sisetemp. 27 °CDB, 19 °CWB; välistemp. 35 °CDB, 24 °CWB; ekvivalentne torustiku pikkus: 5 m","(1) - Jahutus: sisetemp. 27 °CDB, 19 °CWB; välistemp. 35 °CDB, 24 °CWB; ekvivalentne torustiku pikkus: 5 m"]
["","","","","","(2) - Küte: sisetemp. 20 °CDB; välistemp. 7 °CDB, 6 °CWB; ekvivalentne jahutustorustik: 5 m","(2) - Küte: sisetemp. 20 °CDB; välistemp. 7 °CDB, 6 °CWB; ekvivalentne jahutustorustik: 5 m"]
["","","","","","(3) - Vt eraldi elektriandmete joonist","(3) - Vt eraldi elektriandmete joonist"]
["Standardsed lisatarvikud","FTXTP35A5V1B","","","","","1"]