{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":83,"n_cols":7,"rows_kept":83,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTP-K"]
[]
[]
[]
[]
["","","","","","FTXTP25K3V1B","FTXTP35K3V1B"]
["Mürarõhutase","Küte","","kiire","dBA","43"]
["","","","Keskmine","dBA","35"]
["","","","Vaikne töö","dBA","21"]
["","","","aeglane","dBA","26"]
["","Jahutus","","Keskmine","dBA","35"]
["","","","Vaikne töö","dBA","21"]
["","","","aeglane","dBA","26"]
["","","","kiire","dBA","43"]
["Standardsed lisatarvikud","Paigaldusjuhend","","","","1"]
["","Kasutusjuhend","","","","1"]
["","Traadita juhtimispult","","","","1"]
["","AAA kuivelement patareid","","","","2"]
["","Kaugjuhtimispuldi hoidik","","","","1"]
["","Paigaldusplaat","","","","1"]
["","Titaanapatiidist deodoriseeriv filter","","","","2"]
["","Siseseadme kinnituskruvid","","","","2"]
["Juhtsüsteemid","Juhtmega kaugjuhtimine","","","","BRC944B2, BRC073A1"]
["","Infrared remote control","","","","ARC480A11"]
["Toruühendused","Vedelik","","Välisdiameeter","mm","6.35"]
["","Gaas","","Välisdiameeter","mm","9.50"]
["","Tühjendus","","","","16 (ühendusvooliku sisemine läbimõõt)"]
["Sisendvõimsus","Jahutus","","Nom","kW","0.030"]
["","Küte","","Nom","kW","0.035"]
["Müratase","Jahutamine","","","dBA","58"]
["","Soojendamine","","","dBA","58"]
["Mõõtmed","Ühik","","Laius","mm","770"]
["","","","Sügavus","mm","225"]
["","","","Kõrgus","mm","285"]
["Korpus","Värvus","","","","Valge"]
["Kaal","Ühik","","","kg","9.0"]
["Power supply","Faas","","","","1~"]
["","Sagedus","","","Hz","50"]
["","Nimetus","","","","V1"]
["","Pinge","","","V","220-240"]
["Märkused","","","","","(1) - Vt eraldi elektriandmete joonist"]
["Sisendvõimsus","Jahutus","","Nom","kW","","0.03"]
["","Küte","","Nom","kW","","0.035"]
["Korpus","Värvus","","","","","Valge"]
["Mõõtmed","Ühik","","Kõrgus","mm","","285"]
["","","","Laius","mm","","770"]
["","","","Sügavus","mm","","225"]
["Kaal","Ühik","","","kg","","9"]
["Ventilaator","Õhu vooluhulk","Jahutus","kiire","m³/min","","11.4"]
["","Õhuvoolu kiirus","Jahutus","Keskmine","m³/min","","8.2"]
["","","","aeglane","m³/min","","5.4"]
["","","","Vaikne töö","m³/min","","4.3"]
["","","Küte","kiire","m³/min","","10.8"]
["","Õhuvoolu kiirus","Küte","Keskmine","m³/min","","7.8"]
["","","Küte","aeglane","m³/min","","5.8"]
["","","","Vaikne töö","m³/min","","4.9"]
["Helivõimsustase","Jahutamine","","","dBA","","58"]
["","Soojendamine","","","dBA","","58"]
["Mürarõhutase","Jahutus","","kiire","dBA","","43"]
["Helirõhu tase","Jahutus","","Keskmine","dBA","","35"]
["Mürarõhutase","Jahutus","","aeglane","dBA","","26"]
["","","","Vaikne töö","dBA","","21"]
["","Küte","","kiire","dBA","","43"]
["Helirõhu tase","Küte","","Keskmine","dBA","","35"]
["Mürarõhutase","Küte","","aeglane","dBA","","26"]
["","","","Vaikne töö","dBA","","21"]
["Toruühendused","Vedelik","","Välisdiameeter","mm","","6.35"]
["","Gaas","","Välisdiameeter","mm","","9.5"]
["","Tühjendus","","","","","16 (ühendusvooliku sisemine läbimõõt)"]
["Juhtsüsteemid","Infrared remote control","","","","","ARC480A11"]
["Juhtsüsteemid","Juhtmega kaugjuhtimine","","","","","BRC944B2, BRC073A1"]
["Standardsed lisatarvikud","Installation manual","","","","","1"]
["","Wireless remote control","","","","","1"]
["","AAA dry-cell batteries","","","","","2"]
["","Operation manual","","","","","1"]
["","Titanium apatite deodorizing filter","","","","","2"]
["","Indoor unit fixing screws","","","","","2"]
["","Mounting plate","","","","","1"]
["","Remote control holder","","","","","1"]
["Elektritoide","Nimetus","","","","","V1"]
["","Faas","","","","","1~"]
["","Sagedus","","","Hz","","50"]
["","Pinge","","","V","","220-240"]