{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":8,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXZ-N"]
[]
[]
[]
[]
["","","","","","FTXZ25NV1B","FTXZ35NV1B","FTXZ50NV1B"]
["Mürarõhutase","Küte","","kiire","dBA","39","42","44"]
["","","","Vaikne töö","dBA","19","19","24"]
["","","","aeglane","dBA","28","29","31"]
["","Jahutus","","Vaikne töö","dBA","19","19","23"]
["","","","aeglane","dBA","26","27","30"]
["","","","kiire","dBA","38","42","47"]
["","","","Nom","dBA","35","36","38"]
["","Jahutus","","Nom","dBA","33","35","38"]
["Standardsed lisatarvikud","Fotokatalüütiline õhku puhastav ja deodoseeriv filter","","","","1","1","1"]
["","Traadita juhtimispult","","","","1","1","1"]
["","Kuivad akud","","","","2","2","2"]
["","Kaugjuhtimispuldi hoidik","","","","1","1","1"]
["","Siseseadme kinnituskruvid","","","","3","3","3"]
["","Paigaldusplaat","","","","1","1","1"]
["Juhtsüsteemid","Infrared remote control","","","","ARC477A1","ARC477A1","ARC477A1"]
["Toruühendused","Vedelik","","Välisdiameeter","mm","6.35","6.35","6.35"]
["","Gaas","","Välisdiameeter","mm","9.5","9.5","9.5"]
["Power input","Jahutus","","Nom","kW","0.030","0.030","0.030"]
["","Küte","","Nom","kW","0.030","0.030","0.030"]
["Sound power level","Jahutamine","","","dBA","54","57","60"]
["","Soojendamine","","","dBA","56","57","59"]
["Mõõtmed","Ühik","","Laius","mm","798","798","798"]
["","","","Sügavus","mm","372","372","372"]
["","","","Kõrgus","mm","295","295","295"]
["Korpus","Värvus","","","","Valge","Valge","Valge"]
["Kaal","Ühik","","","kg","15","15","15"]
["Ventilaator","Õhu vooluhulk","Küte","kiire","m³/min","11.7","13.3","14.4"]
["","","","aeglane","m³/min","6.7","6.9","7.7"]
["","","","Vaikne töö","m³/min","4.8","4.8","5.9"]
["","","Jahutus","aeglane","m³/min","5.3","5.6","6.6"]
["","","","kiire","m³/min","10.7","12.1","15.0"]
["","","","Vaikne töö","m³/min","4.0","4.0","4.6"]
["","","","Nom","m³/min","8.6","9.2","10.7"]
["","","Jahutus","Nom","m³/min","7.5","8.4","9.2"]
["Power supply","Faas","","","","1~","1~","1~"]
["","Nimetus","","","","V1","V1","V1"]
["","Sagedus","","","Hz","50","50","50"]
["","Pinge","","","V","220-240","220-240","220-240"]
["Märkused","","","","","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230 V","(2) - 230 V","(2) - 230 V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V"]
["","","","","","(4) - Soojusvaheti esiosa","(4) - Soojusvaheti esiosa","(4) - Soojusvaheti esiosa"]
["","","","","","(5) - Soojusvaheti tagaosa","(5) - Soojusvaheti tagaosa","(5) - Soojusvaheti tagaosa"]