{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":82,"n_cols":11,"rows_kept":82,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FUA-A"]
[]
[]
[]
[]
["","","","","","FUA71AVEB9","FUA100AVEB9","FUA125AVEB9","FUA71AVEB (Archived)","FUA100AVEB (Archived)","FUA125AVEB (Archived)"]
["Mürarõhutase","Küte","","kiire","dBA","","","","41","46","47"]
["","","","Keskmine","dBA","","","","38","42","43"]
["","","","aeglane","dBA","","","","35","39","40"]
["","Jahutus","","Keskmine","dBA","","","","38","42","43"]
["","","","aeglane","dBA","","","","35","39","40"]
["","","","kiire","dBA","","","","41","46","47"]
["Standardsed lisatarvikud","Kasutusjuhend","","","","","","","1","1","1"]
["","Paigaldusjuhend","","","","","","","1","1","1"]
["","Tühjendusvoolik","","","","","","","1","1","1"]
["","Torustiku termoisolatsioon","","","","","","","3","3","3"]
["","Kaablisidemed","","","","","","","10","10","10"]
["","Voolikuriba","","","","","","","1","1","1"]
["","Tihendusmaterjal","","","","","","","4","4","4"]
["","Kinnitusplaadi seib","","","","","","","1","1","1"]
["","Tühjendusliitmik","","","","","","","1","1","1"]
["","Lausriie","","","","","","","1","1","1"]
["","Seib","","","","","","","8","8","8"]
["","Tühjendusvooliku kinnituskruvi","","","","","","","5","5","5"]
["Juhtsüsteemid","Juhtmega kaugjuhtimine","","","","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Jahutusvõimsus","Üldvõimsus","","Nom","kW","","","","","","12.1"]
["Piping connections","Vedelik","","Välisdiameeter","mm","","","","9.52","9.52","9.52"]
["","Gaas","","Välisdiameeter","mm","","","","15.9","15.9","15.9"]
["","Tühjendus","","","","","","","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)"]
["Müratase","Jahutamine","","","dBA","","","","59","64","65"]
["","Soojendamine","","","dBA","","","","59","64"]
["Mõõtmed","Seade","","Laius","mm","","","","950","950","950"]
["","","","Sügavus","mm","","","","950","950","950"]
["","","","Kõrgus","mm","","","","198","198","198"]
["Korpus","Materjal","","","","","","","Vaik","Vaik","Vaik"]
["","Värvus","","","","","","","Värske valge","Värske valge","Värske valge"]
["Kaal","Ühik","","","kg","","","","25.0","26.0","26"]
["Ventilaator","Õhu vooluhulk","Küte","kiire","m³/min","","","","23.0","31.0","32.5"]
["","","","Keskmine","m³/min","","","","19.5","25.5","26.5"]
["","","","aeglane","m³/min","","","","16.0","20.0","20.5"]
["","","Jahutus","aeglane","m³/min","","","","16.0","20.0","20.5"]
["","","","Keskmine","m³/min","","","","19.5","25.5","26.5"]
["","","","kiire","m³/min","","","","23.0","31.0","32.5"]
["Tühjenduskõrgus","mm","","","","","","","600","600","600"]
["Küttevõimsus","Üldvõimsus","","Nom.","kW","","","","","","13.5"]
["Korpus","Värvus","","","","Värske valge","Värske valge","Värske valge"]
["","Materjal","","","","Vaik","Vaik","Vaik"]
["Mõõtmed","Ühik","","Kõrgus","mm","198","198","198"]
["","","","Laius","mm","950","950","950"]
["","","","Sügavus","mm","950","950","950"]
["Kaal","Ühik","","","kg","25.0","26.0","26.0"]
["Ventilaator","Õhu vooluhulk","Jahutus","kiire","m³/min","23.0","31.0","32.5"]
["","Õhuvoolu kiirus","Jahutus","Keskmine","m³/min","19.5","25.5","26.5"]
["","","","aeglane","m³/min","16.0","20.0","20.5"]
["","","Küte","kiire","m³/min","23.0","31.0","32.5"]
["","Õhuvoolu kiirus","Küte","Keskmine","m³/min","19.5","25.5","26.5"]
["","","Küte","aeglane","m³/min","16.0","20.0","20.5"]
["Helivõimsustase","Jahutamine","","","dBA","59","64","65"]
["Mürarõhutase","Jahutus","","kiire","dBA","41","46","47"]
["Helirõhu tase","Jahutus","","Keskmine","dBA","38","42","43"]
["Mürarõhutase","Jahutus","","aeglane","dBA","35","39","40"]
["","Küte","","kiire","dBA","41","46","47"]
["Helirõhu tase","Küte","","Keskmine","dBA","38","42","43"]
["Mürarõhutase","Küte","","aeglane","dBA","35","39","40"]
["Toruühendused","Vedelik","","Välisdiameeter","mm","9.52","9.52","9.52"]
["","Gaas","","Välisdiameeter","mm","15.9","15.9","15.9"]
["","Tühjendus","","","","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)"]
["Tühjenduskõrgus","mm","","","","600","600","600"]
["Standardsed lisatarvikud","Installation manual","","","","1","1","1"]
["","Thermal insulation tube","","","","3","3","3"]
["","Non woven fabric","","","","1","1","1"]
["","Drain joint","","","","1","1","1"]
["","Hose band","","","","1","1","1"]
["","Operation manual","","","","1","1","1"]
["","Drain hose","","","","1","1","1"]
["","Fixing screw for drain hose","","","","5","5","5"]
["","Sealing material","","","","4","4","4"]
["","Tie-wraps","","","","10","10","10"]
["","Washer","","","","8","8","8"]
["","Washer fixing plate","","","","1","1","1"]
["Jahutusvõimsus","Üldvõimsus","","Nom","kW","","","12.10"]
["Küttevõimsus","Üldvõimsus","","Nom.","kW","","","13.5"]