{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":45,"n_cols":7,"rows_kept":45,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FUQ-C"]
[]
[]
[]
[]
["","","","","FUQ71CVEB","FUQ100CVEB","FUQ125CVEB"]
["Mürarõhutase","Küte","kiire","dBA","41","46","47"]
["","","Nom","dBA","38","42","43"]
["","","aeglane","dBA","35","39","40"]
["","Jahutus","aeglane","dBA","35","39","40"]
["","","kiire","dBA","41","46","47"]
["","","Nom","dBA","38","42","43"]
["Standardsed lisatarvikud","Paigaldusjuhend","","","Paigaldusjuhend","Paigaldusjuhend","Paigaldusjuhend"]
["","Kasutusjuhend","","","Kasutusjuhend","Kasutusjuhend","Kasutusjuhend"]
["","Vastavusdeklaratsioon","","","Vastavusdeklaratsioon","Vastavusdeklaratsioon","Vastavusdeklaratsioon"]
["","Tühjendusvoolik","","","Tühjendusvoolik","Tühjendusvoolik","Tühjendusvoolik"]
["","Klambri metall","","","Klambri metall","Klambri metall","Klambri metall"]
["","riputuskanduri seib","","","riputuskanduri seib","riputuskanduri seib","riputuskanduri seib"]
["","Klambrid","","","Klambrid","Klambrid","Klambrid"]
["","Seibi klamber","","","Seibi klamber","Seibi klamber","Seibi klamber"]
["","Liitmiku isolatsiooni- ja tihendusmaterjal","","","Liitmiku isolatsiooni- ja tihendusmaterjal","Liitmiku isolatsiooni- ja tihendusmaterjal","Liitmiku isolatsiooni- ja tihendusmaterjal"]
["","Põlv","","","Põlv","Põlv","Põlv"]
["","Paigaldusšabloon","","","Paigaldusšabloon","Paigaldusšabloon","Paigaldusšabloon"]
["","Blokeerimismaterjal","","","Blokeerimismaterjal","Blokeerimismaterjal","Blokeerimismaterjal"]
["","L-kujuline torustik","","","L-kujuline torustik","L-kujuline torustik","L-kujuline torustik"]
["","Kruvid","","","Kruvid","Kruvid","Kruvid"]
["","Lausriie","","","Lausriie","Lausriie","Lausriie"]
["Juhtsüsteemid","Juhtmega kaugjuhtimine","","","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B"]
["","Infrared remote control","","","BRC7C58","BRC7C58","BRC7C58"]
["Toruühendused","Vedelik","Välisdiameeter","mm","9.52","9.52","9.52"]
["","Gaas","Välisdiameeter","mm","15.9","15.9","15.9"]
["","Tühjendus","","","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)"]
["Sound power level","Jahutamine","","dBA","59","64","65"]
["","Soojendamine","","dBA","59","64","65"]
["Mõõtmed","Ühik","Laius","mm","950","950","950"]
["","","Sügavus","mm","950","950","950"]
["","","Kõrgus","mm","198","198","198"]
["Korpus","Materjal","","","Vaik","Vaik","Vaik"]
["","Värvus","","","Värske valge","Värske valge","Värske valge"]
["Kaal","Ühik","","kg","25","26","26"]
["Tühjenduskõrgus","mm","","","600","600","600"]
["Power supply","Faas","","","1~","1~","1~"]
["","Sagedus","","Hz","50/60","50/60","50/60"]
["","Nimetus","","","VE","VE","VE"]
["","Pinge","","V","220-240/220","220-240/220","220-240/220"]