{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":46,"n_cols":9,"rows_kept":46,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVA-A"]
[]
[]
[]
[]
["","","","","","FVA71AMVEB","FVA100AMVEB","FVA125AMVEB","FVA140AMVEB"]
["Jahutusvõimsus","Üldvõimsus","","Nom","kW","","","12.10","13.40"]
["Küttevõimsus","Üldvõimsus","","Nom.","kW","","","13.5","15.5"]
["Korpus","Värvus","","","","Värske valge","Värske valge","Värske valge","Värske valge"]
["Mõõtmed","Ühik","","Kõrgus","mm","1850","1850","1850","1850"]
["","","","Laius","mm","600","600","600","600"]
["","","","Sügavus","mm","270","350","350","350"]
["Kaal","Ühik","","","kg","42","50","50","50"]
["Ventilaator","Õhu vooluhulk","Jahutus","kiire","m³/min","18","28","28","30"]
["","Õhuvoolu kiirus","Jahutus","Keskmine","m³/min","16","25","26","28"]
["","","","aeglane","m³/min","14","22","24","26"]
["","","Küte","kiire","m³/min","18","28","28","30"]
["","Õhuvoolu kiirus","Küte","Keskmine","m³/min","16","25","26","28"]
["","","Küte","aeglane","m³/min","14","22","24","26"]
["Helivõimsustase","Jahutamine","","","dBA","55","62","63","65"]
["Mürarõhutase","Jahutus","","kiire","dBA","43","50","51","53"]
["Helirõhu tase","Jahutus","","Keskmine","dBA","41","47","48","51"]
["Mürarõhutase","Jahutus","","aeglane","dBA","38","44","46","48"]
["","Küte","","kiire","dBA","43","50","51","53"]
["Helirõhu tase","Küte","","Keskmine","dBA","38","44","46","48"]
["Mürarõhutase","Küte","","Nom","dBA","41","47","48","51"]
["Toruühendused","Vedelik","","Välisdiameeter","mm","9.52","9.52","9.52","9.52"]
["","Gaas","","Välisdiameeter","mm","15.9","15.9","15.9","15.9"]
["","Tühjendus","","","","I.D. 20/O.D. 26","I.D. 20/O.D. 26","I.D. 20/O.D. 26","I.D. 20/O.D. 26"]
["Juhtsüsteemid","Juhtmega kaugjuhtimine","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Standardsed lisatarvikud","Installation manual","","","","1","1","1","1"]
["","Hole protection rubber","","","","2","2","2","2"]
["","Cover","","","","1","1","1","1"]
["","Dew proof material","","","","1","1","1","1"]
["","Remote control wiring","","","","1","1","1","1"]
["","Bracket for installation","","","","1","1","1","1"]
["","Operation manual","","","","1","1","1","1"]
["","Bush","","","","1","1","1","1"]
["","Installation pattern","","","","1","1","1","1"]
["","Insulation for fitting for gas pipe","","","","1","1","1","1"]
["","Insulation for fitting for liquid pipe","","","","1","1","1","1"]
["","Screws","","","","5","5","5","5"]
["","Tie-wraps","","","","5","5","5","5"]
["Elektritoide","Faas","","","","1~","1~","1~","1~"]
["","Sagedus","","","Hz","50/60","50/60","50/60","50/60"]
["","Pinge","","","V","220-240/220","220-240/220","220-240/220","220-240/220"]