{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":8,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVQ-C"]
[]
[]
[]
[]
["","","","","FVQ71CVEB","FVQ100CVEB","FVQ125CVEB","FVQ140CVEB"]
["Helirõhu tase","Küte","kiire","dBA","43","50","51","53"]
["","","Nom","dBA","41","47","48","51"]
["","","aeglane","dBA","38","44","46","48"]
["","Jahutus","aeglane","dBA","38","44","46","48"]
["","","kiire","dBA","43","50","51","53"]
["","","Nom","dBA","41","47","48","51"]
["Standardsed lisatarvikud","Kasutusjuhend","","","Kasutusjuhend","Kasutusjuhend","Kasutusjuhend","Kasutusjuhend"]
["","Paigaldusjuhend","","","Paigaldusjuhend","Paigaldusjuhend","Paigaldusjuhend","Paigaldusjuhend"]
["","Paigalduskandur","","","Paigalduskandur","Paigalduskandur","Paigalduskandur","Paigalduskandur"]
["","Kumm ava kaitseks","","","Kumm ava kaitseks","Kumm ava kaitseks","Kumm ava kaitseks","Kumm ava kaitseks"]
["","Hari","","","Hari","Hari","Hari","Hari"]
["","Liitmike isolatsioon","","","Liitmike isolatsioon","Liitmike isolatsioon","Liitmike isolatsioon","Liitmike isolatsioon"]
["","Kate","","","Kate","Kate","Kate","Kate"]
["","Klambrid","","","Klambrid","Klambrid","Klambrid","Klambrid"]
["","Kruvid","","","Kruvid","Kruvid","Kruvid","Kruvid"]
["","Paigaldusšabloon","","","Paigaldusšabloon","Paigaldusšabloon","Paigaldusšabloon","Paigaldusšabloon"]
["","Kastekindel materjal","","","Kastekindel materjal","Kastekindel materjal","Kastekindel materjal","Kastekindel materjal"]
["","Kaugjuhtsüsteemi juhtmestik","","","Kaugjuhtsüsteemi juhtmestik","Kaugjuhtsüsteemi juhtmestik","Kaugjuhtsüsteemi juhtmestik","Kaugjuhtsüsteemi juhtmestik"]
["Control systems","Wired remote control","","","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B"]
["Toruühendused","Vedelik","Välisdiameeter","mm","9.52","9.52","9.52","9.52"]
["","Gaas","Välisdiameeter","mm","15.9","15.9","15.9","15.9"]
["","Drain","","","I.D. 20/O.D. 26","I.D. 20/O.D. 26","I.D. 20/O.D. 26","I.D. 20/O.D. 26"]
["Sisendvõimsus","Jahutus","Nom","kW","0.117","0.238","0.238","0.276"]
["","Küte","Nom","kW","0.117","0.238","0.238","0.276"]
["Müratase","Jahutamine","","dBA","55","62","63","65"]
["","Soojendamine","","dBA","55","62","63","65"]
["Mõõtmed","Ühik","Laius","mm","600","600","600","600"]
["","","Sügavus","mm","270","350","350","350"]
["","","Kõrgus","mm","1,850","1,850","1,850","1,850"]
["Korpus","Colour","","","Värske valge","Värske valge","Värske valge","Värske valge"]
["Kaal","Ühik","","kg","39","47","47","47"]
["Power supply","Phase","","","1~","1~","1~","1~"]
["","Sagedus","","Hz","50/60","50/60","50/60","50/60"]
["","Pinge","","V","220-240/220","220-240/220","220-240/220","220-240/220"]