{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":6,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXG-K / RXLG-M"]
[]
[]
[]
[]
["","","","","FVXG25K2V1B / RXLG25M2V1B","FVXG35K2V1B / RXLG35M2V1B"]
["Jahutusvõimsus","Min","","kW","1.2","1.4"]
["","Max","","kW","5.1","5.6"]
["","Nom","","kW","2.5 (2)","3.5 (2)"]
["Torustikuühendused","Vedelik","Välisdiameeter","mm","6.35","6.35"]
["","Gaas","Välisdiameeter","mm","9.5","9.5"]
["","Tühjendus","OD","mm","18","18"]
["Nominaalne kasutegur","Aastane energiatarve","","kWh","355","510"]
["","Energiatõhususe suhtarv","","","3.52 (1)","3.43 (1)"]
["","COP","","","3.88 (1)","3.61 (1)"]
["","Energiamärgistamise direktiiv","Jahutus","","A","A"]
["","","Küte","","A","A"]
["Küttevõimsus","Nom","","kW","4.5 (2)","5.6 (2)"]
["","Min","","kW","1.0 (6)","1.1 (6)"]
["","Max","","kW","6.5, 3.5 (7)","7.0, 4.0 (7)"]
["Märkused","","","","(1) - EER/COP vastavalt Eurovent 2012-le, kasutamiseks ainult väljaspool EL-i","(1) - EER/COP vastavalt Eurovent 2012-le, kasutamiseks ainult väljaspool EL-i"]
["","","","","(2) - Nimikasutegur: jahutus 35°/27° nominaalkoormusel, küte 7°/20° nominaalkoormusel","(2) - Nimikasutegur: jahutus 35°/27° nominaalkoormusel, küte 7°/20° nominaalkoormusel"]
["","","","","(3) - 220V","(3) - 220V"]
["","","","","(4) - 230 V","(4) - 230 V"]
["","","","","(5) - 240V","(5) - 240V"]
["","","","","(6) - Minimaalse nimikütteväärtuse jaoks on sisepaigaldise ventilaator seadistatud astmele SL","(6) - Minimaalse nimikütteväärtuse jaoks on sisepaigaldise ventilaator seadistatud astmele SL"]
["","","","","(7) - Maksimaalne küttevõimsus -15°C välistemperatuuri juures","(7) - Maksimaalne küttevõimsus -15°C välistemperatuuri juures"]