{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":48,"n_cols":6,"rows_kept":48,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXTM-A"]
[]
[]
[]
[]
["","","","","","FVXTM30A3V1B"]
["Sisendvõimsus","Jahutus","","Nom","kW","0.02"]
["","Küte","","Nom","kW","0.03"]
["Korpus","Värvus","","","","Valge"]
["Mõõtmed","Ühik","","Kõrgus","mm","600"]
["","","","Laius","mm","750"]
["","","","Sügavus","mm","238"]
["Kaal","Ühik","","","kg","17"]
["Ventilaator","Õhu vooluhulk","Jahutus","kiire","m³/min","9"]
["","Õhuvoolu kiirus","Jahutus","Keskmine","m³/min","6.7"]
["","","","aeglane","m³/min","4.8"]
["","","","Vaikne töö","m³/min","4"]
["","","Küte","kiire","m³/min","9.4"]
["","Õhuvoolu kiirus","Küte","Keskmine","m³/min","6.8"]
["","","Küte","aeglane","m³/min","5.3"]
["","","","Vaikne töö","m³/min","4"]
["Helivõimsustase","Jahutamine","","","dBA","53"]
["","Soojendamine","","","dBA","53"]
["Mürarõhutase","Jahutus","","kiire","dBA","39"]
["Helirõhu tase","Jahutus","","Keskmine","dBA","32"]
["Mürarõhutase","Jahutus","","aeglane","dBA","25"]
["","","","Vaikne töö","dBA","20"]
["","Küte","","kiire","dBA","39"]
["Helirõhu tase","Küte","","Keskmine","dBA","32"]
["Mürarõhutase","Küte","","aeglane","dBA","25"]
["","","","Vaikne töö","dBA","19"]
["Külmaaine","GWP","","","","675"]
["Toruühendused","Vedelik","","Välisdiameeter","mm","6.35"]
["","Gaas","","Välisdiameeter","mm","9.5"]
["","Tühjendus","","","","VP20 (I.D. 20/O.D. 26)"]
["Juhtsüsteemid","Infrared remote control","","","","ARC466A66"]
["Juhtsüsteemid","Juhtmega kaugjuhtimine","","","","BRC073A1"]
["Standardsed lisatarvikud","Installation manual","","","","1"]
["","Wireless remote control","","","","1"]
["","AAA dry-cell batteries","","","","2"]
["","General safety precautions","","","","1"]
["","Operation manual","","","","1"]
["","Titanium apatite deodorizing filter","","","","2"]
["","Remote control holder","","","","1"]
["","Screw bag","","","","2"]
["Elektritoide","Faas","","","","1~"]
["","Sagedus","","","Hz","50"]
["","Pinge","","","V","220-240"]